(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.564)
  )
  (paper "User" 200 200)
  (title_block
    (title "MangoPi-MQ")
    (rev "v1.5")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "底层丝印层")
    (37 "F.SilkS" user "顶层丝印层")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.017))
      (layer "dielectric 2" (type "prepreg") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.017))
      (layer "dielectric 3" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "Immersion gold")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 100)
    (grid_origin 100 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "NetP1_2")
  (net 2 "DVP_RST")
  (net 3 "PD22")
  (net 4 "CTP_RST")
  (net 5 "NetR47_1")
  (net 6 "NetC85_1")
  (net 7 "NetC54_2")
  (net 8 "NetDS2_K")
  (net 9 "NetR23_2")
  (net 10 "NetC81_1")
  (net 11 "NetC70_1")
  (net 12 "NetC7_2")
  (net 13 "VCC_RTC")
  (net 14 "TVIN_VRP")
  (net 15 "TVIN_VRN")
  (net 16 "TVIN1")
  (net 17 "TVIN0")
  (net 18 "TV_OUT")
  (net 19 "NetR59_1")
  (net 20 "NetR54_1")
  (net 21 "NetC80_2")
  (net 22 "NetC78_1")
  (net 23 "NetC40_2")
  (net 24 "NetC12_2")
  (net 25 "NetC6_2")
  (net 26 "NetC4_2")
  (net 27 "MICIN3P")
  (net 28 "MICIN3N")
  (net 29 "LINEINR")
  (net 30 "LINEINL")
  (net 31 "AVCC1.8")
  (net 32 "VCC-RMII-CSI")
  (net 33 "NetR50_1")
  (net 34 "NetR35_1")
  (net 35 "DVP_XCLK")
  (net 36 "DVP_VSYNC")
  (net 37 "DVP_SDA")
  (net 38 "DVP_SCL")
  (net 39 "DVP_PCLK")
  (net 40 "DVP_HSYNC")
  (net 41 "DVP_DVDD")
  (net 42 "DVP-Y9")
  (net 43 "DVP-Y8")
  (net 44 "DVP-Y7")
  (net 45 "DVP-Y6")
  (net 46 "DVP-Y5")
  (net 47 "DVP-Y4")
  (net 48 "DVP-Y3")
  (net 49 "DVP-Y2")
  (net 50 "AVDD2V8")
  (net 51 "AAGND")
  (net 52 "PG11")
  (net 53 "CTP_INT")
  (net 54 "WL_REG_ON")
  (net 55 "PB7")
  (net 56 "PB6")
  (net 57 "PB5")
  (net 58 "PB4")
  (net 59 "NetC58_2")
  (net 60 "NetC48_2")
  (net 61 "32I")
  (net 62 "32O")
  (net 63 "XI")
  (net 64 "BT_WAKE_AP")
  (net 65 "BT_EN")
  (net 66 "AP_WAKE_BT")
  (net 67 "D1_P")
  (net 68 "D1_N")
  (net 69 "D0_P")
  (net 70 "D0_N")
  (net 71 "CK_P")
  (net 72 "CK_N")
  (net 73 "NetJ3_B5")
  (net 74 "NetJ3_A5")
  (net 75 "NetJ2_B5")
  (net 76 "NetJ2_A5")
  (net 77 "LCD_PWM")
  (net 78 "LCD_D18")
  (net 79 "NetR39_1")
  (net 80 "WL_WAKE_AP")
  (net 81 "VCC_WIFI")
  (net 82 "UART1_TX")
  (net 83 "UART1_RX")
  (net 84 "UART1_RTS")
  (net 85 "UART1_CTS")
  (net 86 "PG5_SDC1_D3")
  (net 87 "PG4_SDC1_D2")
  (net 88 "PG3_SDC1_D1")
  (net 89 "PG2_SDC1_D0")
  (net 90 "PG1_SDC1_CMD")
  (net 91 "PG0_SDC1_CLK")
  (net 92 "NetR41_2")
  (net 93 "AP-CLK24M-OUT")
  (net 94 "USB1_P")
  (net 95 "USB1_N")
  (net 96 "USB0_P")
  (net 97 "USB0_N")
  (net 98 "TP-Y2")
  (net 99 "TP-Y1")
  (net 100 "TP-X2")
  (net 101 "TP-X1")
  (net 102 "SPI0_WP")
  (net 103 "SPI0_HOLD")
  (net 104 "SDC0_DET")
  (net 105 "RESET")
  (net 106 "NetR49_1")
  (net 107 "NetR43_2")
  (net 108 "HPOUTR")
  (net 109 "HPOUTL")
  (net 110 "HPOUTFB")
  (net 111 "GPADC0")
  (net 112 "VCC-DRAM")
  (net 113 "VCC-CORE")
  (net 114 "XO")
  (net 115 "NetC50_1")
  (net 116 "LDOA-OUT")
  (net 117 "LDO-IN")
  (net 118 "NetR42_2")
  (net 119 "NetR12_2")
  (net 120 "NetR10_2")
  (net 121 "NetR8_2")
  (net 122 "VCCIN")
  (net 123 "VCC3V3")
  (net 124 "NetL3_1")
  (net 125 "NetL2_1")
  (net 126 "NetL1_1")
  (net 127 "NetDS1_K")
  (net 128 "GND")
  (net 129 "AGND")
  (net 130 "LCD_CLK")
  (net 131 "LCD_D10")
  (net 132 "LCD_D11")
  (net 133 "LCD_D12")
  (net 134 "LCD_D13")
  (net 135 "LCD_D14")
  (net 136 "LCD_D15")
  (net 137 "LCD_D19")
  (net 138 "LCD_D20")
  (net 139 "LCD_D21")
  (net 140 "LCD_D22")
  (net 141 "LCD_D23")
  (net 142 "LCD_DE")
  (net 143 "LCD_HSYNC")
  (net 144 "LCD_VSYNC")
  (net 145 "SDC0_CLK")
  (net 146 "SDC0_CMD")
  (net 147 "SDC0_D0")
  (net 148 "SDC0_D1")
  (net 149 "SDC0_D2")
  (net 150 "SDC0_D3")
  (net 151 "SPI0_CLK")
  (net 152 "SPI0_CS")
  (net 153 "SPI0_MISO")
  (net 154 "SPI0_MOSI")
  (net 155 "LEDA")
  (net 156 "LEDK")
  (net 157 "NetD1_A")
  (net 158 "NetC7_1")
  (footprint "LIB_MANGO.IntLib:VLS252010" (layer "F.Cu")
    (tedit 0)
    (at 131.5468 69.6772 180)
    (fp_text reference "L4" (at -1.1811 2.5527 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uH" (at -5.4991 -4.1021 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.950001 0 270) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "2" smd rect (at -0.95 0 270) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "NetD1_A"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 110.7696 76.6114)
    (fp_text reference "R43" (at -0.438003 -1.071994 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "SDC0_CLK") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "NetR43_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 121.6662 70.1344 90)
    (fp_text reference "C69" (at 1.4605 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "TVIN_VRP") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 112.1412 89.921 90)
    (fp_text reference "C30" (at 1.536702 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.060698 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "VCC-DRAM") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 128.6766 70.1344 -90)
    (fp_text reference "C86" (at -1.5367 0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.0353 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "HPOUTFB") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 131.242 78.4148 -90)
    (fp_text reference "TP6" (at -1.2319 0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at 2.7559 0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "LINEINR") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 118.9484 70.1344 -90)
    (fp_text reference "R67" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "PG1_SDC1_CMD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 131.1658 87.5588 180)
    (fp_text reference "C75" (at 0.072215 1.593662 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at 0.072215 -2.851338 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "TP-X1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 116.2814 70.1344 -90)
    (fp_text reference "R69" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "PG3_SDC1_D1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 108.356605 82.7582 -90)
    (fp_text reference "C43" (at -4.318002 2.1336 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at 0.139698 2.24786 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "32O") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "D:_ÏîÄ¿_ADLIB_A.Pc_HDR2X11T" locked (layer "F.Cu")
    (tedit 0)
    (at 120 95.700001)
    (fp_text reference "P3" (at -11.0338 -9.990001 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Header 11X2" (at 10.839191 -0.000005 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at -12.7 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "2" smd rect locked (at -12.7 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "3" smd rect locked (at -10.16 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "USB1_N"))
    (pad "4" smd rect locked (at -10.16 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "USB1_P"))
    (pad "5" smd rect locked (at -7.62 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "DVP_HSYNC"))
    (pad "6" smd rect locked (at -7.62 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "DVP_VSYNC"))
    (pad "7" smd rect locked (at -5.08 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "DVP_PCLK"))
    (pad "8" smd rect locked (at -5.08 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "DVP_XCLK"))
    (pad "9" smd rect locked (at -2.54 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "DVP-Y2"))
    (pad "10" smd rect locked (at -2.54 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DVP-Y3"))
    (pad "11" smd rect locked (at 0 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "DVP-Y4"))
    (pad "12" smd rect locked (at 0 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "DVP-Y5"))
    (pad "13" smd rect locked (at 2.54 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "DVP-Y6"))
    (pad "14" smd rect locked (at 2.54 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "DVP-Y7"))
    (pad "15" smd rect locked (at 5.08 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "DVP-Y8"))
    (pad "16" smd rect locked (at 5.08 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "DVP-Y9"))
    (pad "17" smd rect locked (at 7.62 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "DVP_SCL"))
    (pad "18" smd rect locked (at 7.62 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "DVP_SDA"))
    (pad "19" smd rect locked (at 10.16 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "CTP_RST"))
    (pad "20" smd rect locked (at 10.16 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "CTP_INT"))
    (pad "21" smd rect locked (at 12.7 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "PB4"))
    (pad "22" smd rect locked (at 12.7 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "PB5"))
  )
  (footprint "LIB_MANGO.IntLib:SOD523" (layer "F.Cu")
    (tedit 0)
    (at 131.496 71.7346)
    (fp_text reference "D1" (at -1.079498 1.3081 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "MSK4010" (at -8.953498 -2.8321 180 unlocked) (layer "B.SilkS") hide)
    (pad "A" smd rect (at -0.749999 -0.000002 90) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "NetD1_A"))
    (pad "K" smd rect (at 0.750001 -0.000002 90) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "LEDA"))
  )
  (footprint "LIB_MANGO.IntLib:SOD523" (layer "F.Cu")
    (tedit 0)
    (at 110.3886 85.984)
    (fp_text reference "D2" (at -0.958004 -1.325991 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MSK4010" (at -2.476008 2.8321 unlocked) (layer "F.SilkS") hide)
    (pad "A" smd rect (at -0.749999 -0.000002 90) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "K" smd rect (at 0.750001 -0.000002 90) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "LDO-IN"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 134.7472 69.6772 -90)
    (fp_text reference "R16" (at -1.5367 0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "75R" (at 3.0353 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "NetP1_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "LEDA") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 131.8262 86.1364 90)
    (fp_text reference "C35" (at 1.282697 0.0127 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 134.29 71.252 180)
    (fp_text reference "R17" (at 0.0381 1.5367 unlocked) (layer "F.SilkS") hide)
    (fp_text value "75R" (at 0.0381 -3.0353 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "NetP1_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "LEDA") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 118.034 70.1344 -90)
    (fp_text reference "R68" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "PG2_SDC1_D0") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 113.716 70.1344 -90)
    (fp_text reference "R5" (at 1.282698 0.0127 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -3.0607 0.0127 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "WL_REG_ON") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 119.7612 70.1344 -90)
    (fp_text reference "C10" (at -1.7907 -3.8227 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 3.3147 -6.6167 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 132.8168 86.1364 90)
    (fp_text reference "C36" (at 1.536702 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.060698 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 111.176 79.761 90)
    (fp_text reference "C79" (at 1.8855 0.3869 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -2.5595 0.3869 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "LDOA-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 102.999999 63.700001)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 120.6756 70.1344 90)
    (fp_text reference "C71" (at 1.4605 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "TVIN_VRN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 110.2616 81.412 90)
    (fp_text reference "C9" (at 1.282697 0.012702 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "XI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:HDR1.27-4" (layer "F.Cu")
    (tedit 0)
    (at 136.999997 67.85)
    (fp_text reference "P6" (at -1.733403 -1.478394 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header 4" (at -1.7145 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -1.905 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "TVIN0"))
    (pad "2" thru_hole circle (at -0.635003 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "NetC54_2"))
    (pad "3" thru_hole circle (at 0.635 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "NetC85_1"))
    (pad "4" thru_hole circle (at 1.905 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 129 "AGND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 111.176 81.412 90)
    (fp_text reference "C8" (at 1.282697 0.0127 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "XO") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 115.4432 70.1344 -90)
    (fp_text reference "R66" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "PG5_SDC1_D3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 114.5796 70.1344 -90)
    (fp_text reference "R65" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "PG4_SDC1_D2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 111.4554 68.5088)
    (fp_text reference "R70" (at 1.193802 -0.279402 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC/100K" (at -1.840512 4.178298 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "UART1_CTS") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:HDR1.27-3" (layer "F.Cu")
    (tedit 0)
    (at 137.00018 91.500001)
    (fp_text reference "P8" (at -2.241403 -1.351395 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header 3" (at 0.2921 5.4229 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -1.27 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "2" thru_hole circle (at 0 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "PB6"))
    (pad "3" thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "PB7"))
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 132.6644 78.4148 -90)
    (fp_text reference "TP5" (at -1.2319 0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at 2.7559 0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "LINEINL") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 112.1412 88.016 90)
    (fp_text reference "C26" (at 1.5367 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 107.4676 84.587 90)
    (fp_text reference "C27" (at 1.5367 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 131.242 79.7991 90)
    (fp_text reference "TP2" (at 1.2319 -0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 -0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 103.5306 79.684803)
    (fp_text reference "R6" (at -0.2667 -1.0795 unlocked) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at -0.2667 2.6035 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "NetDS1_K") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 110.7442 85.0442 180)
    (fp_text reference "C68" (at -1.625846 0.456542 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at 0.0381 -2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "LDO-IN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 129.8958 78.4148 -90)
    (fp_text reference "TP7" (at -1.2319 0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at 2.7559 0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "AGND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 111.176 83.6726 -90)
    (fp_text reference "R61" (at -1.73513 0.768988 45 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0R" (at 2.9845 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "VCC_RTC") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "LDOA-OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 103.5306 78.872 180)
    (fp_text reference "R18" (at 1.282698 0.0127 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10K" (at -2.8067 0.012702 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "SDC0_CMD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 113.2588 68.4834)
    (fp_text reference "R14" (at 1.282697 0.0127 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC/100K" (at -3.0607 0.0127 270 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "WL_REG_ON") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:Y3215" (layer "F.Cu")
    (tedit 0)
    (at 106.2484 80.1928 90)
    (fp_text reference "XT1" (at 2.0828 -1.8288 unlocked) (layer "F.SilkS") hide)
    (fp_text value "32.768K CL=12.5pF" (at -2.705182 -12.861527 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.25 0 270) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "32I"))
    (pad "2" smd rect (at 1.25 0 90) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "32O"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 107.4676 82.7582 -90)
    (fp_text reference "C45" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "32I") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 136.999999 95.700001)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 122.6314 70.1344 90)
    (fp_text reference "C70" (at 1.4605 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "NetC70_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:MIPI_CSI_1.0_30PIN" locked (layer "F.Cu")
    (tedit 0)
    (at 136.999999 79.7)
    (fp_text reference "P5" (at -0.855388 -11.166046 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header15-MIPI" (at -1.844832 27.3223 unlocked) (layer "F.SilkS") hide)
    (fp_text user "1" (at -2.862399 -6.9796 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at 1.560002 -6.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "1" smd rect locked (at -1.559997 -6.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "2" smd rect locked (at 1.560002 -5.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "D1_N"))
    (pad "2" smd rect locked (at -1.559997 -5.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "D1_N"))
    (pad "3" smd rect locked (at -1.559997 -4.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "D1_P"))
    (pad "3" smd rect locked (at 1.560002 -4.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "D1_P"))
    (pad "4" smd rect locked (at 1.560002 -4) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "4" smd rect locked (at -1.559997 -4) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "5" smd rect locked (at 1.560002 -2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "CK_N"))
    (pad "5" smd rect locked (at -1.559997 -2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "CK_N"))
    (pad "6" smd rect locked (at 1.560002 -1.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "CK_P"))
    (pad "6" smd rect locked (at -1.559997 -1.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "CK_P"))
    (pad "7" smd rect locked (at -1.559997 -1.000001) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "7" smd rect locked (at 1.560002 -1.000001) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "8" smd rect locked (at 1.560002 0) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "D0_N"))
    (pad "8" smd rect locked (at -1.559997 0) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "D0_N"))
    (pad "9" smd rect locked (at -1.559997 1) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "D0_P"))
    (pad "9" smd rect locked (at 1.560002 1) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "D0_P"))
    (pad "10" smd rect locked (at 1.560002 1.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "10" smd rect locked (at -1.559997 1.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "11" smd rect locked (at 1.560002 2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "DVP_SCL"))
    (pad "11" smd rect locked (at -1.559997 2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "DVP_SCL"))
    (pad "12" smd rect locked (at 1.560002 3.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "DVP_SDA"))
    (pad "12" smd rect locked (at -1.559997 3.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "DVP_SDA"))
    (pad "13" smd rect locked (at 1.560002 4.999997) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "13" smd rect locked (at -1.559997 4.999997) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "14" smd rect locked (at -1.559997 5.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "14" smd rect locked (at 1.560002 5.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "15" smd rect locked (at 1.560002 6.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "15" smd rect locked (at -1.559997 6.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 129.4132 81.8946)
    (fp_text reference "R59" (at -0.0381 -1.4605 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "NetR59_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "LCD_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 125.8572 70.1344 90)
    (fp_text reference "C6" (at -0.248806 -0.400198 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 4.172498 12.496299 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "HPOUTR") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "NetC6_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 134.422824 88.949976)
    (fp_text reference "C73" (at -0.0381 -1.4605 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "TP-Y1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:QFP129P40B1600_1600H160" locked (layer "F.Cu")
    (tedit 0)
    (at 120 79.7 -90)
    (fp_text reference "U1" (at 0.723897 5.0419 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "D1s-eLQFP128" (at -1.3081 -6.769103 90 unlocked) (layer "B.SilkS") hide)
    (fp_text user "46" (at 7.409998 0.799998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "107" (at -8.009997 -2.399996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "71" (at 3.759992 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "43" (at 7.409998 1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "101" (at -8.009997 -4.799991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "1" (at -6.119988 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "126" (at -8.009997 5.199989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "25" (at 3.359993 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "18" (at 0.559999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "59" (at 7.409998 -4.399992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "97" (at -7.889997 -6.400013 90 unlocked) (layer "Eco1.User"))
    (fp_text user "30" (at 5.359989 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "27" (at 4.159991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "51" (at 7.409998 -1.199998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "100" (at -8.009997 -5.19999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "41" (at 7.409998 2.799994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "6" (at -4.119992 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "76" (at 1.759996 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "79" (at 0.559999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "106" (at -8.009997 -2.799995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "61" (at 7.409998 -5.19999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "68" (at 4.95999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "24" (at 2.959994 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "77" (at 1.359997 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "70" (at 4.159991 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "12" (at -1.839997 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "99" (at -7.889997 -5.599989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "36" (at 7.409998 4.79999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "33" (at 7.409998 5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "58" (at 7.409998 -3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "105" (at -8.009997 -3.199994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "88" (at -3.039994 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "48" (at 7.409998 0 90 unlocked) (layer "Eco1.User"))
    (fp_text user "29" (at 4.95999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "23" (at 2.559995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "80" (at 0.159999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "125" (at -8.009997 4.79999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "7" (at -3.719993 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "82" (at -0.639999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "87" (at -2.639995 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "93" (at -5.03999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "11" (at -2.239996 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "28" (at 4.559991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "86" (at -2.239996 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "127" (at -8.009997 5.599988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "21" (at 1.759996 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "95" (at -5.839989 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "8" (at -3.319994 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "116" (at -8.009997 1.199997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "115" (at -8.009997 0.799998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "118" (at -8.009997 1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "129" (at -0.344993 0.083007 -90 unlocked) (layer "Eco1.User"))
    (fp_text user "92" (at -4.639991 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "56" (at 7.409998 -3.199994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "128" (at -8.009997 5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "26" (at 3.759992 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "62" (at 7.409998 -5.599989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "91" (at -4.239992 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "102" (at -8.009997 -4.399992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "53" (at 7.409998 -1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "83" (at -1.039998 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "89" (at -3.439993 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "66" (at 5.759988 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "3" (at -5.31999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "111" (at -8.009997 -0.799999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "F133-eLQFP128" (at -1.070001 0.259994 -90 unlocked) (layer "Eco1.User"))
    (fp_text user "40" (at 7.409998 3.199993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "81" (at -0.24 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "67" (at 5.359989 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "44" (at 7.409998 1.599996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "65" (at 6.160013 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "119" (at -8.009997 2.399995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "110" (at -8.009997 -1.199998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "94" (at -5.439989 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "55" (at 7.409998 -2.799995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "113" (at -8.009997 0 90 unlocked) (layer "Eco1.User"))
    (fp_text user "45" (at 7.409998 1.199997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "19" (at 0.959998 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "38" (at 7.409998 3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "122" (at -8.009997 3.599992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "39" (at 7.409998 3.599992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "57" (at 7.409998 -3.599993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "120" (at -8.009997 2.799994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "109" (at -8.009997 -1.599997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "20" (at 1.359997 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "31" (at 5.759988 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "5" (at -4.519991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "13" (at -1.439997 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "42" (at 7.409998 2.399995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "104" (at -8.009997 -3.599993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "47" (at 7.409998 0.399999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "121" (at -8.009997 3.199993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "54" (at 7.409998 -2.399996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "22" (at 2.159995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "75" (at 2.159995 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "2" (at -5.719989 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "64" (at 7.409998 -6.400013 90 unlocked) (layer "Eco1.User"))
    (fp_text user "114" (at -8.009997 0.399999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "108" (at -8.009997 -1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "78" (at 0.959998 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "117" (at -8.009997 1.599996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "16" (at -0.24 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "9" (at -2.919995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "10" (at -2.639995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "90" (at -3.839993 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "4" (at -4.919991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "34" (at 7.409998 5.599988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "69" (at 4.559991 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "98" (at -7.889997 -5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "15" (at -0.639999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "14" (at -1.039998 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "123" (at -8.009997 3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "50" (at 7.409998 -0.799999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "103" (at -8.009997 -3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "124" (at -8.009997 4.399991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "60" (at 7.409998 -4.799991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "63" (at 7.409998 -5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "74" (at 2.559995 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "49" (at 7.409998 -0.4 90 unlocked) (layer "Eco1.User"))
    (fp_text user "52" (at 7.409998 -1.599997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "96" (at -6.239988 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "37" (at 7.409998 4.399991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "73" (at 2.959994 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "85" (at -1.839997 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "32" (at 6.160013 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "17" (at 0.159999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "112" (at -8.009997 -0.4 90 unlocked) (layer "Eco1.User"))
    (fp_text user "72" (at 3.359993 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "35" (at 7.409998 5.199989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "84" (at -1.439997 -7.649998 unlocked) (layer "Eco1.User"))
    (pad "1" smd oval locked (at -6.199988 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "UART1_TX"))
    (pad "2" smd oval locked (at -5.799989 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "UART1_RX"))
    (pad "3" smd oval locked (at -5.39999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "UART1_RTS"))
    (pad "4" smd oval locked (at -4.99999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "UART1_CTS"))
    (pad "5" smd oval locked (at -4.599991 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "WL_WAKE_AP"))
    (pad "6" smd oval locked (at -4.199992 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "PG11"))
    (pad "7" smd oval locked (at -3.799993 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "SDC0_D1"))
    (pad "8" smd oval locked (at -3.399994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "SDC0_D0"))
    (pad "9" smd oval locked (at -2.999994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "NetR43_2"))
    (pad "10" smd oval locked (at -2.599995 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "SDC0_CMD"))
    (pad "11" smd oval locked (at -2.199996 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "SDC0_D3"))
    (pad "12" smd oval locked (at -1.799997 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "SDC0_D2"))
    (pad "13" smd oval locked (at -1.399998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "SDC0_DET"))
    (pad "14" smd oval locked (at -0.999998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "SPI0_HOLD"))
    (pad "15" smd oval locked (at -0.599999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "SPI0_WP"))
    (pad "16" smd oval locked (at -0.2 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "SPI0_MISO"))
    (pad "17" smd oval locked (at 0.199999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "SPI0_MOSI"))
    (pad "18" smd oval locked (at 0.599998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "SPI0_CS"))
    (pad "19" smd oval locked (at 0.999998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "NetR49_1"))
    (pad "20" smd oval locked (at 1.399997 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "LDOA-OUT"))
    (pad "21" smd oval locked (at 1.799996 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "AP-CLK24M-OUT"))
    (pad "22" smd oval locked (at 2.199995 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "XO"))
    (pad "23" smd oval locked (at 2.599994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "XI"))
    (pad "24" smd oval locked (at 2.999994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "32O"))
    (pad "25" smd oval locked (at 3.399993 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "32I"))
    (pad "26" smd oval locked (at 3.799992 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "VCC_RTC"))
    (pad "27" smd oval locked (at 4.199991 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "RESET"))
    (pad "28" smd oval locked (at 4.59999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "LDOA-OUT"))
    (pad "29" smd oval locked (at 4.99999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "LDO-IN"))
    (pad "30" smd oval locked (at 5.399989 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "NetC50_1"))
    (pad "31" smd oval locked (at 5.799988 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "DVP_SDA"))
    (pad "32" smd oval locked (at 6.199987 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "DVP_SCL"))
    (pad "33" smd oval locked (at 7.649997 6.199987 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "DVP_XCLK"))
    (pad "34" smd oval locked (at 7.649997 5.799988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "VCC-RMII-CSI"))
    (pad "35" smd oval locked (at 7.649997 5.399989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "DVP_PCLK"))
    (pad "36" smd oval locked (at 7.649997 4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "DVP-Y9"))
    (pad "37" smd oval locked (at 7.649997 4.59999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "DVP-Y8"))
    (pad "38" smd oval locked (at 7.649997 4.199991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "DVP-Y7"))
    (pad "39" smd oval locked (at 7.649997 3.799992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "DVP-Y6"))
    (pad "40" smd oval locked (at 7.649997 3.399993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "DVP-Y5"))
    (pad "41" smd oval locked (at 7.649997 2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "DVP-Y4"))
    (pad "42" smd oval locked (at 7.649997 2.599994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DVP-Y3"))
    (pad "43" smd oval locked (at 7.649997 2.199995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "DVP-Y2"))
    (pad "44" smd oval locked (at 7.649997 1.799996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "DVP_HSYNC"))
    (pad "45" smd oval locked (at 7.649997 1.399997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "DVP_VSYNC"))
    (pad "46" smd oval locked (at 7.649997 0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "VCC-CORE"))
    (pad "47" smd oval locked (at 7.649997 0.599998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "NetR42_2"))
    (pad "48" smd oval locked (at 7.649997 0.199999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "VCC-DRAM"))
    (pad "49" smd oval locked (at 7.649997 -0.2 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "VCC-DRAM"))
    (pad "50" smd oval locked (at 7.649997 -0.599999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "LDOA-OUT"))
    (pad "51" smd oval locked (at 7.649997 -0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "VCC-CORE"))
    (pad "52" smd oval locked (at 7.649997 -1.399998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "PD22"))
    (pad "53" smd oval locked (at 7.649997 -1.799997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "LCD_VSYNC"))
    (pad "54" smd oval locked (at 7.649997 -2.199996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "LCD_HSYNC"))
    (pad "55" smd oval locked (at 7.649997 -2.599995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "D0_P"))
    (pad "56" smd oval locked (at 7.649997 -2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "D0_N"))
    (pad "57" smd oval locked (at 7.649997 -3.399994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "D1_P"))
    (pad "58" smd oval locked (at 7.649997 -3.799993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "D1_N"))
    (pad "59" smd oval locked (at 7.649997 -4.199992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "CK_P"))
    (pad "60" smd oval locked (at 7.649997 -4.599991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "CK_N"))
    (pad "61" smd oval locked (at 7.649997 -4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "LCD_D10"))
    (pad "62" smd oval locked (at 7.649997 -5.39999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "LCD_D11"))
    (pad "63" smd oval locked (at 7.649997 -5.799989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "LCD_D12"))
    (pad "64" smd oval locked (at 7.649997 -6.199988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "LCD_D13"))
    (pad "65" smd oval locked (at 6.199987 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "LDOA-OUT"))
    (pad "66" smd oval locked (at 5.799988 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "67" smd oval locked (at 5.399989 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "LCD_D14"))
    (pad "68" smd oval locked (at 4.99999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "LCD_D15"))
    (pad "69" smd oval locked (at 4.59999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "LCD_D19"))
    (pad "70" smd oval locked (at 4.199991 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LCD_D18"))
    (pad "71" smd oval locked (at 3.799992 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "LCD_D20"))
    (pad "72" smd oval locked (at 3.399993 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "LCD_D21"))
    (pad "73" smd oval locked (at 2.999994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "LCD_D22"))
    (pad "74" smd oval locked (at 2.599994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "LCD_D23"))
    (pad "75" smd oval locked (at 2.199995 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "NetR59_1"))
    (pad "76" smd oval locked (at 1.799996 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "LCD_DE"))
    (pad "77" smd oval locked (at 1.399997 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "NetC12_2"))
    (pad "78" smd oval locked (at 0.999998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "TV_OUT"))
    (pad "79" smd oval locked (at 0.599998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "PB7"))
    (pad "80" smd oval locked (at 0.199999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "PB6"))
    (pad "81" smd oval locked (at -0.2 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "VCC-CORE"))
    (pad "82" smd oval locked (at -0.599999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "PB5"))
    (pad "83" smd oval locked (at -0.999998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "84" smd oval locked (at -1.399998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "PB4"))
    (pad "85" smd oval locked (at -1.799997 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "CTP_INT"))
    (pad "86" smd oval locked (at -2.199996 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "CTP_RST"))
    (pad "87" smd oval locked (at -2.599995 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "MICIN3P"))
    (pad "88" smd oval locked (at -2.999994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "MICIN3N"))
    (pad "89" smd oval locked (at -3.399994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "AVCC1.8"))
    (pad "90" smd oval locked (at -3.799993 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "NetC78_1"))
    (pad "91" smd oval locked (at -4.199992 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "AGND"))
    (pad "92" smd oval locked (at -4.599991 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "NetC40_2"))
    (pad "93" smd oval locked (at -4.99999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "94" smd oval locked (at -5.39999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "95" smd oval locked (at -5.799989 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "LINEINR"))
    (pad "96" smd oval locked (at -6.199988 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "LINEINL"))
    (pad "97" smd oval locked (at -7.649998 -6.199988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "AVCC1.8"))
    (pad "98" smd oval locked (at -7.649998 -5.799989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "HPOUTR"))
    (pad "99" smd oval locked (at -7.649998 -5.39999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "HPOUTL"))
    (pad "100" smd oval locked (at -7.649998 -4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "HPOUTFB"))
    (pad "101" smd oval locked (at -7.649998 -4.599991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "GPADC0"))
    (pad "102" smd oval locked (at -7.649998 -4.199992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "TP-X1"))
    (pad "103" smd oval locked (at -7.649998 -3.799993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "TP-X2"))
    (pad "104" smd oval locked (at -7.649998 -3.399994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "TP-Y1"))
    (pad "105" smd oval locked (at -7.649998 -2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "TP-Y2"))
    (pad "106" smd oval locked (at -7.649998 -2.599995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "NetR54_1"))
    (pad "107" smd oval locked (at -7.649998 -2.199996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "NetC70_1"))
    (pad "108" smd oval locked (at -7.649998 -1.799997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "TVIN0"))
    (pad "109" smd oval locked (at -7.649998 -1.399998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "TVIN1"))
    (pad "110" smd oval locked (at -7.649998 -0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "TVIN_VRP"))
    (pad "111" smd oval locked (at -7.649998 -0.599999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "TVIN_VRN"))
    (pad "112" smd oval locked (at -7.649998 -0.2 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "USB1_P"))
    (pad "113" smd oval locked (at -7.649998 0.199999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "USB1_N"))
    (pad "114" smd oval locked (at -7.649998 0.599998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "USB0_N"))
    (pad "115" smd oval locked (at -7.649998 0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "USB0_P"))
    (pad "116" smd oval locked (at -7.649998 1.399997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "VCC-CORE"))
    (pad "117" smd oval locked (at -7.649998 1.799996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "VCC-CORE"))
    (pad "118" smd oval locked (at -7.649998 2.199995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "PG1_SDC1_CMD"))
    (pad "119" smd oval locked (at -7.649998 2.599994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "PG2_SDC1_D0"))
    (pad "120" smd oval locked (at -7.649998 2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "NetR39_1"))
    (pad "121" smd oval locked (at -7.649998 3.399993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "PG3_SDC1_D1"))
    (pad "122" smd oval locked (at -7.649998 3.799992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "PG5_SDC1_D3"))
    (pad "123" smd oval locked (at -7.649998 4.199991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "PG4_SDC1_D2"))
    (pad "124" smd oval locked (at -7.649998 4.59999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "WL_REG_ON"))
    (pad "125" smd oval locked (at -7.649998 4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "AP_WAKE_BT"))
    (pad "126" smd oval locked (at -7.649998 5.399989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "BT_WAKE_AP"))
    (pad "127" smd oval locked (at -7.649998 5.799988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "BT_EN"))
    (pad "128" smd oval locked (at -7.649998 6.199987 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "129" smd rect locked (at 0 0 270) (size 5.720004 5.720004) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0603" (layer "F.Cu")
    (tedit 0)
    (at 133.7058 69.6772 90)
    (fp_text reference "C1" (at 0.6223 -0.9525 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF 50V" (at -3.0353 -0.9525 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.635 0 270) (size 0.8001 0.849884) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "LEDA"))
    (pad "2" smd rect (at 0.635 0 270) (size 0.8001 0.849884) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0603 SMD Capacitor.STEP"
      (offset (xyz -0.000041 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 115.9004 68.5088)
    (fp_text reference "C18" (at 1.161003 2.103006 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC" (at -0.856973 0.713499 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "PG0_SDC1_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 133.8074 85.2728 90)
    (fp_text reference "C3" (at -1.7653 1.2573 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -5.829295 -2.7813 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 103.5306 80.523)
    (fp_text reference "C41" (at 1.5367 -0.1143 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 -0.1143 270 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 117.1196 70.1344 90)
    (fp_text reference "R39" (at 1.452994 -0.057003 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "NetR39_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "PG0_SDC1_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 120.0406 68.5088)
    (fp_text reference "R41" (at -0.438003 -1.071994 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC/0R" (at -1.3843 2.4003 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "AP-CLK24M-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "NetR41_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:LED0402" (layer "F.Cu")
    (tedit 0)
    (at 101.27 79.6848)
    (fp_text reference "DS1" (at 2.0701 -0.419102 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "GREEN" (at -3.5941 -0.419102 270 unlocked) (layer "F.SilkS") hide)
    (pad "A" smd rect (at -0.507998 0 90) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "K" smd rect (at 0.507997 0 90) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "NetDS1_K"))
  )
  (footprint "LIB_MANGO.IntLib:QFN40P300X300X80_HS-21N" locked (layer "F.Cu")
    (tedit 0)
    (at 109.625601 88.917596 90)
    (fp_text reference "U4" (at -0.749298 2.8067 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "RY1303" (at -6.8453 -4.3307 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd oval locked (at -1.525001 -0.8 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "2" smd oval locked (at -1.525001 -0.400001 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "NetR12_2"))
    (pad "3" smd oval locked (at -1.525001 0 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "NetR10_2"))
    (pad "4" smd oval locked (at -1.525001 0.4 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "5" smd oval locked (at -1.525001 0.799999 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "6" smd oval locked (at -0.800001 1.524999 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "NetL3_1"))
    (pad "7" smd oval locked (at -0.400002 1.524999 90) (size 0.2 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "8" smd oval locked (at 0 1.524999 90) (size 0.2 0.635) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NetR23_2"))
    (pad "9" smd oval locked (at 0.399999 1.524999 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "10" smd oval locked (at 0.799998 1.524999 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "11" smd oval locked (at 1.524998 0.799999 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "NetL1_1"))
    (pad "12" smd oval locked (at 1.524998 0.4 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "13" smd oval locked (at 1.524998 0 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "14" smd oval locked (at 1.524998 -0.400001 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "NetR8_2"))
    (pad "15" smd oval locked (at 1.524998 -0.8 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "16" smd oval locked (at 0.799998 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "17" smd oval locked (at 0.399999 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "18" smd oval locked (at 0 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "NetC4_2"))
    (pad "19" smd oval locked (at -0.400002 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "20" smd oval locked (at -0.800001 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "NetL2_1"))
    (pad "21" smd rect locked (at 0 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:USB-TYPEC-16P" locked (layer "F.Cu")
    (tedit 0)
    (at 103.6 72.199999 -90)
    (fp_text reference "J3" (at -0.170401 7.5184 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB-TypeC-16P" (at 6.4897 0.5207 unlocked) (layer "F.SilkS") hide)
    (pad "0" thru_hole oval locked (at 4.319999 2.547501) (size 1.4 1) (drill oval 1 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "0" thru_hole oval locked (at 4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "0" thru_hole oval locked (at -4.319999 2.547501) (size 1.4 1) (drill oval 1 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "0" thru_hole oval locked (at -4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "A1" smd rect locked (at -3.4 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "A4" smd rect locked (at -2.599999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "A5" smd rect locked (at -1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "NetJ3_A5"))
    (pad "A6" smd rect locked (at -0.249999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "USB0_P"))
    (pad "A7" smd rect locked (at 0.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "USB0_N"))
    (pad "A8" smd rect locked (at 1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A9" smd rect locked (at 2.6 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "A12" smd rect locked (at 3.400001 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "B1" smd rect locked (at 3.099999 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "B4" smd rect locked (at 2.300001 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "B5" smd rect locked (at 1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "NetJ3_B5"))
    (pad "B6" smd rect locked (at 0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "USB0_P"))
    (pad "B7" smd rect locked (at -0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "USB0_N"))
    (pad "B8" smd rect locked (at -1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B9" smd rect locked (at -2.3 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "B12" smd rect locked (at -3.099998 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 109.271 82.7582 -90)
    (fp_text reference "R40" (at -1.071994 0.438003 unlocked) (layer "F.SilkS") hide)
    (fp_text value "680K 1%" (at 2.9845 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "32O") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "32I") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 127.7368 70.1344 -90)
    (fp_text reference "C85" (at -1.5367 0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.0353 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "NetC85_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "HPOUTR") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 113.081 89.921 -90)
    (fp_text reference "C31" (at 1.5367 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 112.7762 70.1344 -90)
    (fp_text reference "C34" (at 1.5367 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 129.8958 79.7991 90)
    (fp_text reference "TP1" (at 1.2319 -0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 -0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "TV_OUT") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 109.271 84.587 -90)
    (fp_text reference "C50" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at 2.9845 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "NetC50_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 124.9174 70.1344 90)
    (fp_text reference "C49" (at 1.5367 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at -3.0607 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "GPADC0") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:USB-TYPEC-16P" locked (layer "F.Cu")
    (tedit 0)
    (at 103.6 87.2 -90)
    (fp_text reference "J2" (at -5.691594 4.952403 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB-TypeC-16P" (at 6.4897 0.5207 unlocked) (layer "F.SilkS") hide)
    (pad "0" thru_hole oval locked (at -4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "0" thru_hole oval locked (at 4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "0" thru_hole oval locked (at 4.319999 2.547501) (size 1.4 1) (drill oval 1 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "0" thru_hole oval locked (at -4.319999 2.547501) (size 1.4 1) (drill oval 1 0.6) (layers *.Cu *.Mask)
      (net 128 "GND"))
    (pad "A1" smd rect locked (at -3.400001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "A4" smd rect locked (at -2.6 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "A5" smd rect locked (at -1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "NetJ2_A5"))
    (pad "A6" smd rect locked (at -0.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "USB1_P"))
    (pad "A7" smd rect locked (at 0.249999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "USB1_N"))
    (pad "A8" smd rect locked (at 1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A9" smd rect locked (at 2.6 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "A12" smd rect locked (at 3.400001 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "B1" smd rect locked (at 3.099999 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "B4" smd rect locked (at 2.3 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "B5" smd rect locked (at 1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "NetJ2_B5"))
    (pad "B6" smd rect locked (at 0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "USB1_P"))
    (pad "B7" smd rect locked (at -0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "USB1_N"))
    (pad "B8" smd rect locked (at -1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B9" smd rect locked (at -2.300001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "B12" smd rect locked (at -3.099999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 131.1658 88.4478 180)
    (fp_text reference "C74" (at 0.28796 2.114517 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at 0.28796 -2.330483 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "TP-X2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:LED0402" (layer "F.Cu")
    (tedit 0)
    (at 131.165797 90.5814)
    (fp_text reference "DS2" (at -0.1651 -1.6637 unlocked) (layer "F.SilkS") hide)
    (fp_text value "BLUE" (at 0.596654 3.1877 unlocked) (layer "F.SilkS") hide)
    (pad "A" smd rect (at -0.507997 0 90) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "K" smd rect (at 0.507998 0 90) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "NetDS2_K"))
  )
  (footprint "LIB_MANGO.IntLib:MIC" locked (layer "F.Cu")
    (tedit 0)
    (at 131.2674 75.443)
    (fp_text reference "M1" (at -1.8669 -2.8829 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MIC" (at -1.8669 4.4069 unlocked) (layer "F.SilkS") hide)
    (fp_text user "" (at -0.508 1.524 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0.7874 -0.4826 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 158 "NetC7_1"))
    (pad "2" thru_hole circle locked (at -0.7874 -0.4826 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "NetC7_2"))
  )
  (footprint "LIB_MANGO.IntLib:I-PEX SOCKET" locked (layer "F.Cu")
    (tedit 0)
    (at 109.4234 71.3028 180)
    (fp_text reference "J4" (at 1.301603 2.773794 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ipex" (at 1.7653 -3.8481 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at 0 1.549999 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "NetC48_2"))
    (pad "2" smd rect locked (at 1.4 0 270) (size 2.2 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "3" smd rect locked (at -1.399999 0 270) (size 2.2 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 131.1658 89.3876 180)
    (fp_text reference "R80" (at -0.8763 1.536705 unlocked) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at -0.8763 -3.035295 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.457197 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "NetDS2_K") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "PD22") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 129.6164 70.1344 90)
    (fp_text reference "C55" (at -1.5367 -3.949705 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 3.0607 -5.219705 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 107.3406 76.6114 180)
    (fp_text reference "R48" (at -2.186274 -0.506812 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0.672895 -2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "SDC0_DET") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 127.9654 87.5588)
    (fp_text reference "C20" (at -1.7907 -3.8227 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 -6.6167 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 136.999999 63.700001)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 110.312402 83.6726 90)
    (fp_text reference "C44" (at 1.4732 -0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "LDOA-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 102.999999 95.700001)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 134.422824 89.8956)
    (fp_text reference "C72" (at -0.0381 -1.4605 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "TP-Y2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 108.3566 84.587 -90)
    (fp_text reference "R8" (at -0.520697 -1.1303 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "680K 1%" (at -0.5207 2.9083 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "NetR8_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "D:_×ÊÁÏ¿â_ADLIB_A.PcbLib_HDR2X11T" locked (layer "F.Cu")
    (tedit 0)
    (at 120 63.700001)
    (fp_text reference "P2" (at -0.990188 -4.310047 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header 11X2" (at -3.047014 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at -12.7 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "2" smd rect locked (at -12.7 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "VCC3V3"))
    (pad "3" smd rect locked (at -10.16 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "PG0_SDC1_CLK"))
    (pad "4" smd rect locked (at -10.16 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "PG1_SDC1_CMD"))
    (pad "5" smd rect locked (at -7.62 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "PG2_SDC1_D0"))
    (pad "6" smd rect locked (at -7.62 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "PG3_SDC1_D1"))
    (pad "7" smd rect locked (at -5.08 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "PG4_SDC1_D2"))
    (pad "8" smd rect locked (at -5.08 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "PG5_SDC1_D3"))
    (pad "9" smd rect locked (at -2.54 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "UART1_TX"))
    (pad "10" smd rect locked (at -2.54 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "UART1_RX"))
    (pad "11" smd rect locked (at 0 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "UART1_RTS"))
    (pad "12" smd rect locked (at 0 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "UART1_CTS"))
    (pad "13" smd rect locked (at 2.54 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "WL_WAKE_AP"))
    (pad "14" smd rect locked (at 2.54 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "PG11"))
    (pad "15" smd rect locked (at 5.08 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "WL_REG_ON"))
    (pad "16" smd rect locked (at 5.08 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "AP_WAKE_BT"))
    (pad "17" smd rect locked (at 7.62 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "BT_WAKE_AP"))
    (pad "18" smd rect locked (at 7.62 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "BT_EN"))
    (pad "19" smd rect locked (at 10.16 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "PD22"))
    (pad "20" smd rect locked (at 10.16 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "GPADC0"))
    (pad "21" smd rect locked (at 12.7 2.749997) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "VCCIN"))
    (pad "22" smd rect locked (at 12.7 -2.750002) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 126.7716 70.1344 90)
    (fp_text reference "R3" (at 1.282697 0.0127 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "NetC6_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 112.6238 91.2418 180)
    (fp_text reference "R10" (at 1.536703 -0.114298 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "300K 1%" (at -3.3147 -0.114298 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "VCC-DRAM") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "NetR10_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:XTAL2520" (layer "F.Cu")
    (tedit 0)
    (at 108.7122 80.1928 90)
    (fp_text reference "X1" (at -0.325006 -0.273198 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XTAL2520-24M CL=18PF" (at -8.612899 -2.633698 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.8636 -0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "XO"))
    (pad "2" smd rect (at -0.8636 -0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
    (pad "3" smd rect (at -0.8636 0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "XI"))
    (pad "4" smd rect (at 0.8636 0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 124.0284 70.1344 -90)
    (fp_text reference "R29" (at 1.5367 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -3.0607 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "GPADC0") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 108.1788 63.1494 -90)
    (fp_text reference "C16" (at -1.7907 3.568698 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 6.3627 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "VCC_WIFI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 117.7546 73.2332)
    (fp_text reference "C39" (at 1.282697 -0.0127 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -2.8067 -0.012702 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 130.861 75.9764 180)
    (fp_text reference "C7" (at -0.4953 1.0795 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100pF" (at -2.018807 -2.324182 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 158 "NetC7_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "NetC7_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 115.4686 91.5974 -90)
    (fp_text reference "C63" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "AAGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "AVDD2V8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 105.9182 71.861603 180)
    (fp_text reference "R78" (at -0.0381 1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -0.0381 -3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 154 "SPI0_MOSI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:FPC6" locked (layer "B.Cu")
    (tedit 0)
    (at 129.9974 63.378 180)
    (fp_text reference "P4" (at 0.5842 0.330197 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "FPC6" (at 30.2641 7.9883 270 unlocked) (layer "F.SilkS") hide)
    (pad "0" smd rect locked (at -3.300001 1.383792) (size 1.6 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "0" smd rect locked (at 3.300001 1.391874) (size 1.6 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "1" smd rect locked (at -1.25002 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "CTP_RST"))
    (pad "2" smd oval locked (at -0.750021 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
    (pad "3" smd oval locked (at -0.250022 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "4" smd oval locked (at 0.249977 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "CTP_INT"))
    (pad "5" smd oval locked (at 0.749976 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "DVP_SDA"))
    (pad "6" smd oval locked (at 1.249975 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "DVP_SCL"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 104.5974 70.6424 -90)
    (fp_text reference "R28" (at -1.026398 -0.474698 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at 3.409496 -0.4631 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "NetJ3_A5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:VLS2016" (layer "B.Cu")
    (tedit 0)
    (at 111.0744 90.4036 90)
    (fp_text reference "L3" (at -0.8509 1.7145 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uH" (at -0.8509 -3.2385 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.675 0) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "NetL3_1"))
    (pad "2" smd rect (at -0.675 0) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "VCC-DRAM"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 127.6098 71.6076 90)
    (fp_text reference "C54" (at 1.5367 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0353 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 109 "HPOUTL") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "NetC54_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 110.4648 94.579401 90)
    (fp_text reference "C64" (at 1.4732 0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "AVDD2V8") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "AAGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 128.829 73.538 90)
    (fp_text reference "R55" (at 0.521756 -0.864388 unlocked) (layer "B.SilkS") hide)
    (fp_text value "75R" (at -3.4925 0.2921 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "AVCC1.8") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "NetC81_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 129.9212 73.538 -90)
    (fp_text reference "C81" (at -1.244844 3.326824 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "NetC81_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 122.4028 82.9614 90)
    (fp_text reference "R76" (at 1.5367 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -3.0353 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 153 "SPI0_MISO") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 124.2824 72.0394 -90)
    (fp_text reference "C22" (at -1.7907 3.8227 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at 3.3147 6.3627 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 129.1338 75.9764 180)
    (fp_text reference "C47" (at -0.0381 1.4605 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -1.434648 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "NetC7_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "MICIN3N") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 103.8354 87.4572 -90)
    (fp_text reference "C84" (at -7.491697 -5.804908 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.046697 -5.804908 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 105 "RESET") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 123.0124 61.0666 90)
    (fp_text reference "R47" (at 1.452994 0.044597 unlocked) (layer "B.SilkS") hide)
    (fp_text value "47K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "NetR47_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 125.5016 72.0394 90)
    (fp_text reference "C80" (at 1.035499 0.4631 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.409501 0.4631 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 109 "HPOUTL") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "NetC80_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 122.0218 87.3556 180)
    (fp_text reference "C77" (at -0.476179 1.023488 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -0.4699 -3.4163 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 116 "LDOA-OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 114.5542 91.5974 90)
    (fp_text reference "R53" (at 1.4732 0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "AAGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 118.600001 87.299195 90)
    (fp_text reference "C38" (at 1.282698 -0.0127 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -2.8067 -0.012703 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 106.096 93.1468 180)
    (fp_text reference "C65" (at -0.0508 1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -0.0381 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 121.8694 76.4082 90)
    (fp_text reference "C42" (at 1.071994 3.625997 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 125.3238 77.9576)
    (fp_text reference "C2" (at -1.7653 -1.2573 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -5.8293 2.7813 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 104.597395 72.3188 90)
    (fp_text reference "R30" (at 1.451394 0.049697 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "NetJ3_B5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 104.698997 88.8542 90)
    (fp_text reference "C76" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TFCARD-1040310811" locked (layer "B.Cu")
    (tedit 0)
    (at 102.5 79.7 90)
    (fp_text reference "J1" (at 0.3048 0.2286 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TF5033981892" (at -8.3947 2.705097 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at 3.105 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "SDC0_D2"))
    (pad "2" smd rect locked (at 2.005 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 150 "SDC0_D3"))
    (pad "3" smd rect locked (at 0.905 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "SDC0_CMD"))
    (pad "4" smd rect locked (at -0.195001 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
    (pad "5" smd rect locked (at -1.295001 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 145 "SDC0_CLK"))
    (pad "6" smd rect locked (at -2.394999 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "7" smd rect locked (at -3.494999 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "SDC0_D0"))
    (pad "8" smd rect locked (at -4.544999 0.239499 90) (size 0.75 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "SDC0_D1"))
    (pad "G1" smd rect locked (at 5.565001 0.3645 90) (size 1.55 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "G2" smd rect locked (at -5.755 0.589498 90) (size 1.17 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "G3" smd rect locked (at -3.73 11.074999 90) (size 1.9 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "G4" smd rect locked (at 2.240001 11.074999 90) (size 1.9 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "G5" smd rect locked (at 5.740002 10.1 90) (size 1.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "G6" smd rect locked (at 5.740002 6.4 90) (size 1.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "SDC0_DET"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 103.683 70.6424 -90)
    (fp_text reference "C83" (at -1.522697 -0.089908 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 2.922303 -0.089908 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 120.5994 86.0602 -90)
    (fp_text reference "C21" (at -4.872799 5.982198 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -1.558099 6.129902 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 112 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 124.917402 61.0666 -90)
    (fp_text reference "R82" (at -1.5367 -0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at 3.0353 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "CTP_INT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 119.6596 91.572 -90)
    (fp_text reference "C61" (at -1.8982 -0.4758 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.5595 -0.4631 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "AAGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 105.9182 87.9398)
    (fp_text reference "R1" (at -1.384298 -1.2573 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -1.8923 2.781298 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "NetC4_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 123.4696 62.5906 180)
    (fp_text reference "R84" (at -0.0381 1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 1.358448 -3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "PG11") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "NetR47_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:MINISW" locked (layer "B.Cu")
    (tedit 0)
    (at 101 88.699999 -90)
    (fp_text reference "S2" (at 3.5941 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "SW-CE" (at -5.0927 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (pad "0" smd rect locked (at -2.3 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "0" smd rect locked (at 2.300001 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "1" smd rect locked (at -1.675 -1.55 270) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "RESET"))
    (pad "2" smd rect locked (at 1.675001 -1.55 90) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 107.4168 87.635 -135)
    (fp_text reference "R45" (at -0.466977 1.706252 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 2.765915 -1.52664 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.457197 0.000001 225) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "NetR23_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.457202 0.000002 225) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "NetC4_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.02539998269 -0.004001517275 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 126.771597 70.1344 -90)
    (fp_text reference "C5" (at -1.7653 -1.2573 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -5.8293 2.7813 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 127.599198 86.034798)
    (fp_text reference "C13" (at -1.7907 3.5687 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 6.3627 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.457199 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 116 "LDOA-OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 108.7376 87 -90)
    (fp_text reference "C25" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 114.605 81.539 90)
    (fp_text reference "TP3" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "VCC_RTC") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 128.2194 91.572 90)
    (fp_text reference "R73" (at 1.478394 0.057002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "DVP_SDA") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 125.3238 78.9482)
    (fp_text reference "C53" (at 0.0508 -1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 0.0381 2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 115.5194 85.5776 180)
    (fp_text reference "R74" (at 0.062492 1.624297 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at 0.062492 -2.820703 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 116 "LDOA-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 105 "RESET") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 132.9184 72.268 90)
    (fp_text reference "C60" (at -1.5367 3.949705 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.0607 5.219707 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 126.162 91.572 90)
    (fp_text reference "R35" (at 1.505869 0.147962 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -2.951831 0.135262 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "NetR35_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 119.3802 86.0602 -90)
    (fp_text reference "C52" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 112 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 127.4066 73.7158 -90)
    (fp_text reference "R15" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -3.0607 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 125.8572 70.1344 90)
    (fp_text reference "R64" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "33R" (at -2.9845 -0.723654 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "NetC80_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 107.569197 92.461)
    (fp_text reference "R12" (at 1.5367 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "75K 1%" (at -3.3147 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 119 "NetR12_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23" (layer "B.Cu")
    (tedit 0)
    (at 108.197603 94.579398 -90)
    (fp_text reference "U9" (at -2.064593 -1.694592 unlocked) (layer "B.SilkS") hide)
    (fp_text value "XC6206-2.8" (at 4.475907 -1.707292 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at -0.949998 -1.174997 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "AAGND"))
    (pad "2" smd rect (at 0.950001 -1.175002 270) (size 0.899998 0.950011) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "AVDD2V8"))
    (pad "3" smd rect (at 0.000003 1.175004 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 125.250005 91.572 90)
    (fp_text reference "R50" (at 1.262258 -1.465234 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -3.195442 -1.477934 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "NetR50_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "D:_×ÊÁÏ¿â_ADLIB_A.PcbLib_AP6212" locked (layer "B.Cu")
    (tedit 0)
    (at 116.000001 66.300001)
    (fp_text reference "U6" (at 6.140597 -7.167994 unlocked) (layer "B.SilkS") hide)
    (fp_text value "WIFI" (at -2.412221 0 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd oval locked (at -5.699999 4.499999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "2" smd oval locked (at -5.699999 3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "NetC58_2"))
    (pad "3" smd oval locked (at -5.699999 2.699997 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "4" smd oval locked (at -5.699999 1.799999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd oval locked (at -5.699999 0.900001 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "6" smd oval locked (at -5.699999 0 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "AP_WAKE_BT"))
    (pad "7" smd oval locked (at -5.699999 -0.900001 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "BT_WAKE_AP"))
    (pad "8" smd oval locked (at -5.699999 -1.799999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "9" smd oval locked (at -5.699999 -2.699997 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "VCC_WIFI"))
    (pad "10" smd oval locked (at -5.699999 -3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "11" smd oval locked (at -5.699999 -4.499999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "12" smd oval locked (at -4.499999 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "WL_REG_ON"))
    (pad "13" smd oval locked (at -3.599998 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "WL_WAKE_AP"))
    (pad "14" smd oval locked (at -2.699997 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "PG4_SDC1_D2"))
    (pad "15" smd oval locked (at -1.799999 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "PG5_SDC1_D3"))
    (pad "16" smd oval locked (at -0.900001 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "PG1_SDC1_CMD"))
    (pad "17" smd oval locked (at 0 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "PG0_SDC1_CLK"))
    (pad "18" smd oval locked (at 0.9 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "PG2_SDC1_D0"))
    (pad "19" smd oval locked (at 1.799999 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "PG3_SDC1_D1"))
    (pad "20" smd oval locked (at 2.699997 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "21" smd oval locked (at 3.599998 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "22" smd oval locked (at 4.499998 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
    (pad "23" smd oval locked (at 5.699998 -4.499999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "24" smd oval locked (at 5.699998 -3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "NetR47_1"))
    (pad "25" smd oval locked (at 5.699998 -2.699997 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "26" smd oval locked (at 5.699998 -1.799999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "27" smd oval locked (at 5.699998 -0.900001 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "28" smd oval locked (at 5.699998 0 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "29" smd oval locked (at 5.699998 0.900001 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "30" smd oval locked (at 5.699998 1.799999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "NetR41_2"))
    (pad "31" smd oval locked (at 5.699998 2.699997 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "32" smd oval locked (at 5.699998 3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "33" smd oval locked (at 5.699998 4.499999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "34" smd oval locked (at 4.499998 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "BT_EN"))
    (pad "35" smd oval locked (at 3.599998 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "36" smd oval locked (at 2.699997 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "37" smd oval locked (at 1.799999 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "38" smd oval locked (at 0.9 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "39" smd oval locked (at 0 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "40" smd oval locked (at -0.900001 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "41" smd oval locked (at -1.799999 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "UART1_CTS"))
    (pad "42" smd oval locked (at -2.699997 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "UART1_RX"))
    (pad "43" smd oval locked (at -3.599998 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "UART1_TX"))
    (pad "44" smd oval locked (at -4.499999 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "UART1_RTS"))
    (pad "TP1" smd circle locked (at -2.7 3.6 270) (size 0.254 0.254) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "TP2" smd circle locked (at -0.900001 3.6 270) (size 0.254 0.254) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "TP3" smd circle locked (at 0.9 3.6 270) (size 0.254 0.254) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "LIB_MANGO.IntLib:SOT23" locked (layer "B.Cu")
    (tedit 0)
    (at 108.2042 97.7696 -90)
    (fp_text reference "U8" (at -2.5146 -1.2446 unlocked) (layer "B.SilkS") hide)
    (fp_text value "XC6206-1.2" (at 4.0259 -7.09741 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at -0.949998 -1.174996 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "2" smd rect locked (at 0.950001 -1.175001 270) (size 0.899998 0.950011) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "DVP_DVDD"))
    (pad "3" smd rect locked (at 0.000003 1.175004 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 109.625601 90.3782 90)
    (fp_text reference "R11" (at 1.536702 0.114298 unlocked) (layer "B.SilkS") hide)
    (fp_text value "150K 1%" (at -3.3147 0.1143 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 120 "NetR10_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 117.400006 87.299197 90)
    (fp_text reference "R42" (at 1.452994 0.057002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "240R 1%" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 118 "NetR42_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 127.258421 91.572 90)
    (fp_text reference "R72" (at 1.478394 0.057003 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "DVP_SCL") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 105.9182 88.8288 180)
    (fp_text reference "R2" (at -1.8923 -1.257298 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -1.8923 2.781297 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "NetC4_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 114.0716 89.0066 90)
    (fp_text reference "R57" (at 1.071994 0.438002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -2.5781 0.4445 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 114.5034 87.4572 180)
    (fp_text reference "C66" (at -0.0508 1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -0.0381 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 105.9182 87.0508)
    (fp_text reference "R23" (at -0.8763 -1.536695 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100K" (at -0.8763 3.035305 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.457197 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "NetR23_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 105.9182 89.7432)
    (fp_text reference "C4" (at -1.7653 -1.2573 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -5.8293 2.7813 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "NetC4_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 132.0548 73.538 -90)
    (fp_text reference "R27" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1K" (at -3.060702 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "NetC81_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 158 "NetC7_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 109.0932 68.712 -90)
    (fp_text reference "C58" (at -0.757052 1.327661 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 2.9845 1.993242 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "NetC58_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 107.2644 63.1494 90)
    (fp_text reference "R58" (at 1.473205 -0.8128 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -2.984495 -0.8255 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "VCC_WIFI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 132.5628 66.934 180)
    (fp_text reference "R81" (at -0.0381 1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -0.0381 -3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "CTP_RST") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23" locked (layer "B.Cu")
    (tedit 0)
    (at 123.9522 74.554 -90)
    (fp_text reference "U2" (at -1.2827 -2.5019 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XC6206-1.8V" (at -7.3787 4.0259 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at -0.949998 -1.174996 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "AGND"))
    (pad "2" smd rect locked (at 0.950001 -1.175001 270) (size 0.899998 0.950011) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "AVCC1.8"))
    (pad "3" smd rect locked (at 0.000003 1.175004 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 130.0482 76.8146 180)
    (fp_text reference "C46" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 158 "NetC7_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "MICIN3P") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 116.383 91.5974 90)
    (fp_text reference "R52" (at 1.4732 0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "DVP_RST") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 105 "RESET") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 129.6926 71.8108)
    (fp_text reference "R32" (at 1.536697 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -3.0607 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "PD22") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "LCD_PWM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 107.5946 91.5212)
    (fp_text reference "C32" (at 1.5367 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 109.2456 92.461 180)
    (fp_text reference "R13" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "150K 1%" (at -3.3147 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 119 "NetR12_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 115.5194 84.7394)
    (fp_text reference "R7" (at 1.282697 -0.0127 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -2.8067 -0.012702 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 152 "SPI0_CS") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 125.3238 80.9548)
    (fp_text reference "C12" (at -1.7907 3.5687 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 6.3627 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "NetC12_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23-6" locked (layer "B.Cu")
    (tedit 0)
    (at 131.7086 69.687401 180)
    (fp_text reference "U5" (at -0.952508 -2.5527 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MT9284-28J" (at -6.794503 4.3053 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at -1.000001 0.950001 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "NetD1_A"))
    (pad "2" smd rect locked (at -1.000001 0 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "3" smd rect locked (at -1.000001 -0.949998 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "LEDK"))
    (pad "4" smd rect locked (at 1 -0.949998 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "LCD_PWM"))
    (pad "5" smd rect locked (at 1 0 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "LEDA"))
    (pad "6" smd rect locked (at 1 0.950001 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "VCCIN"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 107.747 69.1692)
    (fp_text reference "C48" (at 0.044597 -1.452997 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 0.0381 2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "NetC48_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 120.0406 73.2332 180)
    (fp_text reference "R37" (at -0.0508 1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100K" (at 2.247161 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "BT_EN") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 123.1902 72.0394 -90)
    (fp_text reference "R71" (at -1.198989 -1.174602 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at 2.984505 -0.9017 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "NetC70_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:WSON-SPIFLASH" locked (layer "B.Cu")
    (tedit 0)
    (at 118.288 79.7102 90)
    (fp_text reference "U3" (at -0.571503 -3.289298 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SPIFLASH_SOP8W" (at -17.310103 5.2451 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval locked (at -3.764001 1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "SPI0_CS"))
    (pad "2" smd oval locked (at -3.764001 0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 153 "SPI0_MISO"))
    (pad "3" smd oval locked (at -3.764001 -0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "SPI0_WP"))
    (pad "4" smd rect locked (at 0 0 90) (size 3.4 4.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "4" smd oval locked (at -3.764001 -1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "5" smd oval locked (at 3.764 -1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "SPI0_MOSI"))
    (pad "6" smd oval locked (at 3.764 -0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 151 "SPI0_CLK"))
    (pad "7" smd oval locked (at 3.764 0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "SPI0_HOLD"))
    (pad "8" smd oval locked (at 3.764 1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 130.5308 66.934)
    (fp_text reference "C51" (at 1.5367 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 123.2664 82.3518 -90)
    (fp_text reference "R75" (at -1.5367 -0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at 3.0353 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 153 "SPI0_MISO") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 103.683 72.3188 90)
    (fp_text reference "C82" (at 7.390099 5.957308 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 2.945099 5.957308 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 125.3238 79.9388)
    (fp_text reference "R60" (at 0.057002 -1.452994 unlocked) (layer "B.SilkS") hide)
    (fp_text value "75R" (at 0.0381 2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "TV_OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 117.2212 84.7394 180)
    (fp_text reference "R33" (at 0.812551 -5.155545 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -0.0381 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 102 "SPI0_WP") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 121.1582 74.5286 -90)
    (fp_text reference "R54" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC/1K" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "NetR54_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 109.0932 63.1494 -90)
    (fp_text reference "C14" (at -1.7907 3.822703 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.3147 6.362703 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "VCC_WIFI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 105.9182 72.776003)
    (fp_text reference "R77" (at 0.0381 -1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 0.0381 3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 154 "SPI0_MOSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 114.986 89.0066 -90)
    (fp_text reference "R56" (at -1.0668 -0.4572 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at 2.5781 -0.4445 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "AVDD2V8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 134.2646 69.5248 -90)
    (fp_text reference "R4" (at -0.520697 1.1303 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2R7" (at -0.520697 -2.6543 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 156 "LEDK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 108.6614 69.9058 180)
    (fp_text reference "R38" (at -0.438002 1.071994 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -0.6477 -3.1369 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "NetC58_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "NetC48_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 121.8186 86.0602 -90)
    (fp_text reference "C37" (at -1.15998 0.687421 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 3.28502 0.687421 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 106.223 86.238 180)
    (fp_text reference "R9" (at -0.520697 1.1303 unlocked) (layer "B.SilkS") hide)
    (fp_text value "150K 1%" (at -0.5207 -2.9083 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 121 "NetR8_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 131.0642 73.538 90)
    (fp_text reference "R34" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1K" (at -2.9845 -0.850613 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "NetC7_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 134.0106 72.268 -90)
    (fp_text reference "C59" (at -1.2827 4.0767 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 2.806703 3.8227 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 109.6266 87 90)
    (fp_text reference "C29" (at 1.5367 0.1143 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 126.4668 73.7158 -90)
    (fp_text reference "C40" (at 1.282698 -0.0127 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.47uF" (at -2.8067 -0.012702 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "NetC40_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 110.4648 97.769603 -90)
    (fp_text reference "C62" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "DVP_DVDD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:VLS2016" (layer "B.Cu")
    (tedit 0)
    (at 107.7978 90.2004)
    (fp_text reference "L2" (at -0.8509 1.714503 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uH" (at -0.8509 -3.238502 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.675 0 270) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "NetL2_1"))
    (pad "2" smd rect (at -0.675 0 270) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "VCC-CORE"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 120.1422 87.381)
    (fp_text reference "C24" (at 1.282697 -0.0127 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1uF" (at -2.8067 -0.012702 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 112 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 117.5006 74.6048)
    (fp_text reference "R49" (at 2.034776 2.309965 unlocked) (layer "B.SilkS") hide)
    (fp_text value "33R" (at -0.386901 2.559505 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "NetR49_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 151 "SPI0_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 103.835402 90.2004 -90)
    (fp_text reference "R26" (at 2.024548 -0.686047 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at 3.176303 0.164091 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "NetJ2_B5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 129.2354 69.7026 -90)
    (fp_text reference "C23" (at -1.5367 3.949705 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.0607 5.219708 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 127.4066 75.3922 90)
    (fp_text reference "C78" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.47uF" (at -2.9845 0.672894 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "NetC78_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 125.3238 81.8946 180)
    (fp_text reference "R79" (at 0.8128 1.473205 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at 0.8255 -2.984495 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "NetC12_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 119.5834 74.6048 180)
    (fp_text reference "R25" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -3.0607 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 103 "SPI0_HOLD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 131.496 71.8108 180)
    (fp_text reference "R36" (at 0.158603 -1.010806 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at 0.5715 -5.0673 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "LCD_PWM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 126.466802 75.3922 90)
    (fp_text reference "C11" (at 1.5367 0.1143 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uF" (at -3.0607 0.1143 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "AVCC1.8") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 123.901402 61.0666 90)
    (fp_text reference "C19" (at -0.241206 0.600596 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1uF" (at -2.008902 5.418105 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 114.6812 83.444 90)
    (fp_text reference "TP4" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 104.699 86.9492 -90)
    (fp_text reference "R24" (at -1.453652 0.577751 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at -2.691102 -6.553304 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "NetJ2_A5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:FFC{slash}SM0.5-2H24-OV5640" locked (layer "B.Cu")
    (tedit 0)
    (at 120 95.199999 180)
    (fp_text reference "U7" (at -1.421989 -1.879354 unlocked) (layer "B.SilkS") hide)
    (fp_text value "OV-DVP" (at -1.977126 -5.559725 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at 5.74997 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd rect locked (at 5.249971 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "AAGND"))
    (pad "3" smd rect locked (at 4.749972 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "DVP_SDA"))
    (pad "4" smd rect locked (at 4.249973 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "AVDD2V8"))
    (pad "5" smd rect locked (at 3.749974 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "DVP_SCL"))
    (pad "6" smd rect locked (at 3.249975 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "DVP_RST"))
    (pad "7" smd rect locked (at 2.749976 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "DVP_VSYNC"))
    (pad "8" smd rect locked (at 2.249977 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "9" smd rect locked (at 1.749978 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "DVP_HSYNC"))
    (pad "10" smd rect locked (at 1.249979 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "DVP_DVDD"))
    (pad "11" smd rect locked (at 0.74998 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "VCC-RMII-CSI"))
    (pad "12" smd rect locked (at 0.249981 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "DVP-Y9"))
    (pad "13" smd rect locked (at -0.250018 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "DVP_XCLK"))
    (pad "14" smd rect locked (at -0.750017 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "DVP-Y8"))
    (pad "15" smd rect locked (at -1.250016 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "16" smd rect locked (at -1.750015 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "DVP-Y7"))
    (pad "17" smd rect locked (at -2.250014 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "DVP_PCLK"))
    (pad "18" smd rect locked (at -2.750013 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "DVP-Y6"))
    (pad "19" smd rect locked (at -3.250012 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "DVP-Y2"))
    (pad "20" smd rect locked (at -3.750011 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "DVP-Y5"))
    (pad "21" smd rect locked (at -4.25001 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "DVP-Y3"))
    (pad "22" smd rect locked (at -4.750009 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "DVP-Y4"))
    (pad "23" smd rect locked (at -5.250008 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "NetR50_1"))
    (pad "24" smd rect locked (at -5.750007 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "NetR35_1"))
    (pad "P0" smd rect locked (at 7.649984 -1.625001 270) (size 2.2 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "P0" smd rect locked (at -7.649985 -1.625001 270) (size 2.2 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 109.1186 66.6546 -90)
    (fp_text reference "R46" (at -1.048199 0.374206 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC/100K" (at 3.409501 -3.294903 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "AP_WAKE_BT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:FFC{slash}SM0.5-1H40" locked (layer "B.Cu")
    (tedit 0)
    (at 136.999999 79.7 -90)
    (fp_text reference "P1" (at 24.5745 1.9685 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "FFC40-RGBLCD" (at -3.2385 1.9685 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at -9.749986 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "LEDK"))
    (pad "2" smd rect locked (at -9.249987 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "NetP1_2"))
    (pad "3" smd rect locked (at -8.749988 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "4" smd rect locked (at -8.249989 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
    (pad "5" smd rect locked (at -7.74999 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "6" smd rect locked (at -7.249991 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "7" smd rect locked (at -6.749992 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "LCD_D18"))
    (pad "8" smd rect locked (at -6.249993 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "LCD_D19"))
    (pad "9" smd rect locked (at -5.749994 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "LCD_D20"))
    (pad "10" smd rect locked (at -5.249995 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "LCD_D21"))
    (pad "11" smd rect locked (at -4.749996 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "LCD_D22"))
    (pad "12" smd rect locked (at -4.249997 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "LCD_D23"))
    (pad "13" smd rect locked (at -3.749998 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "14" smd rect locked (at -3.249999 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "15" smd rect locked (at -2.75 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "LCD_D10"))
    (pad "16" smd rect locked (at -2.250001 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "LCD_D11"))
    (pad "17" smd rect locked (at -1.750002 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "LCD_D12"))
    (pad "18" smd rect locked (at -1.250003 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "LCD_D13"))
    (pad "19" smd rect locked (at -0.750004 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "LCD_D14"))
    (pad "20" smd rect locked (at -0.250005 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "LCD_D15"))
    (pad "21" smd rect locked (at 0.249994 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "22" smd rect locked (at 0.749993 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "23" smd rect locked (at 1.249992 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "D0_P"))
    (pad "24" smd rect locked (at 1.749991 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "D0_N"))
    (pad "25" smd rect locked (at 2.24999 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "D1_P"))
    (pad "26" smd rect locked (at 2.749989 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "D1_N"))
    (pad "27" smd rect locked (at 3.249988 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "CK_P"))
    (pad "28" smd rect locked (at 3.749987 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "CK_N"))
    (pad "29" smd rect locked (at 4.249986 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "30" smd rect locked (at 4.749985 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "LCD_CLK"))
    (pad "31" smd rect locked (at 5.249984 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
    (pad "32" smd rect locked (at 5.749983 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "LCD_HSYNC"))
    (pad "33" smd rect locked (at 6.249982 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 144 "LCD_VSYNC"))
    (pad "34" smd rect locked (at 6.749981 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "LCD_DE"))
    (pad "35" smd rect locked (at 7.24998 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
    (pad "36" smd rect locked (at 7.749979 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "37" smd rect locked (at 8.249978 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "TP-X1"))
    (pad "38" smd rect locked (at 8.749977 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "TP-Y1"))
    (pad "39" smd rect locked (at 9.249976 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "TP-X2"))
    (pad "40" smd rect locked (at 9.749975 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "TP-Y2"))
    (pad "G" smd rect locked (at 10.635003 -1.405098 180) (size 1.15 0.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "G" smd rect locked (at -10.634998 -1.405098 180) (size 1.15 0.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:VLS2016" (layer "B.Cu")
    (tedit 0)
    (at 111.1506 87.217597 -90)
    (fp_text reference "L1" (at 0.248806 -0.285602 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uH" (at -4.1699 0.740098 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.675 0 180) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "NetL1_1"))
    (pad "2" smd rect (at -0.675 0 180) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 112.6746 87 -90)
    (fp_text reference "C28" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:MINISW" locked (layer "B.Cu")
    (tedit 0)
    (at 101 70.7 -90)
    (fp_text reference "S1" (at 3.5941 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "SW-CE" (at -5.0927 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (pad "0" smd rect locked (at -2.300001 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "0" smd rect locked (at 2.3 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "1" smd rect locked (at -1.675001 -1.55 270) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "GND"))
    (pad "2" smd rect locked (at 1.675 -1.55 90) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "SPI0_MOSI"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 118.7452 91.572 90)
    (fp_text reference "C67" (at 1.452994 0.057002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "DVP_DVDD") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 107.5946 88.7526 180)
    (fp_text reference "C33" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 128 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (gr_line (start 106.499999 100) (end 133.499999 100) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 105.499999 60.700002) (end 102.999999 60.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 134.499999 98.7) (end 136.999999 98.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 139.999999 95.700001) (mid 139.121319 97.821321) (end 136.999999 98.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 100 63.700001) (end 100 95.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -114.534603 212.521606) (end -114.534603 212.521606) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 106.499999 99.7) (end 106.499999 100) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -114.534603 212.521606) (end -114.534603 212.521606) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 100 95.700001) (end 99.999999 95.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 133.499999 59.4) (end 106.499999 59.4) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 136.999999 60.700002) (end 134.499999 60.700002) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 102.999999 98.700001) (mid 100.878679 97.821321) (end 99.999999 95.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 139.999998 95.700001) (end 139.999996 63.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -114.534603 212.521606) (end -114.534603 212.521606) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -114.534603 212.521606) (end -114.534603 212.521606) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 102.999999 98.7) (end 105.499999 98.7) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 99.999999 63.700001) (mid 100.878679 61.578681) (end 102.999999 60.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 136.999998 60.700004) (mid 139.121316 61.578683) (end 139.999994 63.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 106.499999 59.4) (end 106.499999 59.700002) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 133.499999 99.7) (end 134.499999 98.7) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 139.999996 63.700001) (end 139.999994 63.700001) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 136.999997 60.700005) (end 136.999999 60.700002) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 134.499999 60.700002) (end 133.499999 59.700002) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 133.499999 100) (end 133.499999 99.7) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 105.499999 98.7) (end 106.499999 99.7) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 106.499999 59.700002) (end 105.499999 60.700002) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 133.499999 59.700002) (end 133.499999 59.4) (layer "Edge.Cuts") (width 0.05))
  (gr_text "DVP" (at 122.0472 92.7102) (layer "B.SilkS"))
  (gr_text "IN0" (at 135.687 67.2086) (layer "B.SilkS"))
  (gr_text "mangopi.org" (at 130.4546 93.2182) (layer "B.SilkS"))
  (gr_text "+" (at 114.097 80.9246) (layer "B.SilkS"))
  (gr_text "LO" (at 136.9316 67.2086) (layer "B.SilkS"))
  (gr_text "CTP" (at 129.337 67.2086) (layer "B.SilkS"))
  (gr_text "R3" (at 138.989 92.8118) (layer "B.SilkS"))
  (gr_text "T3" (at 137.6174 92.8118) (layer "B.SilkS"))
  (gr_text "FEL" (at 102.413 70.7392 270) (layer "B.SilkS"))
  (gr_text "G" (at 139.2938 67.2086) (layer "B.SilkS"))
  (gr_text "RST" (at 102.3114 88.824 270) (layer "B.SilkS"))
  (gr_text "RO" (at 138.3286 67.2086) (layer "B.SilkS"))
  (gr_text "G" (at 136.0934 92.8118) (layer "B.SilkS"))
  (gr_text "TF" (at 100.9398 80.1626 270) (layer "B.SilkS"))
  (gr_text "G" (at 135.3314 92.8372) (layer "F.SilkS"))
  (gr_text "13" (at 123.1394 67.220596) (layer "F.SilkS"))
  (gr_text "8" (at 115.796346 61.155993) (layer "F.SilkS"))
  (gr_text "L" (at 133.2486 78.6688) (layer "F.SilkS"))
  (gr_text "IN0" (at 134.3154 67.222948) (layer "F.SilkS"))
  (gr_text "19" (at 130.7594 67.271396) (layer "F.SilkS"))
  (gr_text "R3" (at 137.7952 92.8118) (layer "F.SilkS"))
  (gr_text "P3" (at 122.7584 96.426245) (layer "F.SilkS"))
  (gr_text "T3" (at 136.4998 92.8118) (layer "F.SilkS"))
  (gr_text "7" (at 115.802158 67.221135) (layer "F.SilkS"))
  (gr_text "G" (at 128.8544 78.634957) (layer "F.SilkS"))
  (gr_text "X" (at 122.3774 89.713) (layer "F.SilkS"))
  (gr_text "Nezha-MQ" (at 130.9626 83.0836 45) (layer "F.SilkS"))
  (gr_text "OTG" (at 100.4064 77.902) (layer "F.SilkS"))
  (gr_text "HOST" (at 100.508 82.2454) (layer "F.SilkS"))
  (gr_text "8" (at 115.796346 93.001068) (layer "F.SilkS"))
  (gr_text "RO" (at 137.084 67.227523) (layer "F.SilkS"))
  (gr_text "14" (at 123.140985 61.164985) (layer "F.SilkS"))
  (gr_text "7" (at 115.802158 99.277222) (layer "F.SilkS"))
  (gr_text "G" (at 138.608 67.227523) (layer "F.SilkS"))
  (gr_text "LO" (at 135.814 67.227523) (layer "F.SilkS"))
  (gr_text "MangoPi" (at 117.5514 89.713) (layer "F.SilkS"))
  (gr_text "14" (at 123.140985 93.010059) (layer "F.SilkS"))
  (gr_text "13" (at 123.1394 99.276684) (layer "F.SilkS"))
  (gr_text "G" (at 131.8262 80.031957) (layer "F.SilkS"))
  (gr_text "19" (at 130.7594 99.327484) (layer "F.SilkS"))
  (gr_text "2" (at 107.983415 61.164985) (layer "F.SilkS"))
  (gr_text "ANT" (at 108.2042 73.9904) (layer "F.SilkS"))
  (gr_text "V1.5-211125" (at 132.1056 83.7186 45) (layer "F.SilkS"))
  (gr_text "PWM7" (at 132.1818 90.8354) (layer "F.SilkS"))
  (gr_text "1" (at 108.128 67.229059) (layer "F.SilkS"))
  (gr_text "2" (at 107.983415 93.010059) (layer "F.SilkS"))
  (gr_text "1" (at 108.128 99.285147) (layer "F.SilkS"))
  (gr_text "20" (at 130.706743 93.001068) (layer "F.SilkS"))
  (gr_text "20" (at 130.706743 61.155993) (layer "F.SilkS"))
  (gr_text "TV" (at 128.6766 79.9848) (layer "F.SilkS"))
  (gr_text "P2" (at 124.257 64.14) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 100 63.700001) (xy 139.999994 63.700001))
    (height -9.547001)
    (gr_text "40.0000 mm" (at 119.999997 52.003) (layer "F.SilkS"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.05) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 133.499999 59.700002) (xy 133.499999 99.7))
    (height -11.813601)
    (gr_text "40.0000 mm" (at 143.1636 79.700001 90) (layer "F.SilkS"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.05) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.0449 60.655101)
        (xy 137.063499 60.700002)
        (xy 137.0449 60.744903)
        (xy 136.999999 60.763502)
        (xy 134.499999 60.763502)
        (xy 134.455098 60.744903)
        (xy 134.436499 60.700002)
        (xy 134.455098 60.655101)
        (xy 134.499999 60.636502)
        (xy 136.999999 60.636502)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.0449 95.6551)
        (xy 140.063499 95.700001)
        (xy 140.046717 96.020224)
        (xy 139.996554 96.336938)
        (xy 139.91356 96.646674)
        (xy 139.798645 96.946039)
        (xy 139.653068 97.231751)
        (xy 139.478422 97.500681)
        (xy 139.276623 97.749882)
        (xy 139.04988 97.976625)
        (xy 138.800679 98.178424)
        (xy 138.531749 98.35307)
        (xy 138.246037 98.498647)
        (xy 137.946672 98.613562)
        (xy 137.636936 98.696556)
        (xy 137.320222 98.746719)
        (xy 136.999999 98.763501)
        (xy 136.955098 98.744902)
        (xy 136.936499 98.700001)
        (xy 136.955098 98.6551)
        (xy 136.999999 98.636501)
        (xy 137.009836 98.640576)
        (xy 137.329301 98.622635)
        (xy 137.654461 98.567388)
        (xy 137.971392 98.476082)
        (xy 138.276106 98.349865)
        (xy 138.564773 98.190324)
        (xy 138.833761 97.999466)
        (xy 139.07969 97.779692)
        (xy 139.299464 97.533763)
        (xy 139.490322 97.264775)
        (xy 139.649863 96.976108)
        (xy 139.77608 96.671394)
        (xy 139.867386 96.354463)
        (xy 139.922633 96.029303)
        (xy 139.940574 95.709838)
        (xy 139.936499 95.700001)
        (xy 139.955098 95.6551)
        (xy 139.999999 95.636501)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.800005 80.999997)
        (xy 118.64999 80.999997)
        (xy 118.64999 80.799997)
        (xy 117.800005 80.799997)
        (xy 117.800005 79.799999)
        (xy 118.64999 79.799999)
        (xy 118.64999 79.6)
        (xy 117.849992 79.6)
        (xy 117.800005 79.6)
        (xy 117.800005 78.600002)
        (xy 117.849992 78.600002)
        (xy 118.64999 78.600002)
        (xy 118.64999 78.400002)
        (xy 117.800005 78.400002)
        (xy 117.800005 77.500004)
        (xy 118.700003 77.500004)
        (xy 118.700003 78.34999)
        (xy 118.900003 78.34999)
        (xy 118.900003 77.500004)
        (xy 119.900001 77.500004)
        (xy 119.900001 78.34999)
        (xy 120.1 78.34999)
        (xy 120.1 77.500004)
        (xy 121.099998 77.500004)
        (xy 121.099998 78.34999)
        (xy 121.299998 78.34999)
        (xy 121.299998 77.500004)
        (xy 122.199996 77.500004)
        (xy 122.199996 78.400002)
        (xy 118.700003 78.400002)
        (xy 118.700003 79.549987)
        (xy 118.900003 79.549987)
        (xy 118.900003 78.600002)
        (xy 119.900001 78.600002)
        (xy 119.900001 79.549987)
        (xy 120.1 79.549987)
        (xy 120.1 78.600002)
        (xy 121.099998 78.600002)
        (xy 121.099998 79.549987)
        (xy 121.299998 79.549987)
        (xy 121.299998 78.600002)
        (xy 122.199996 78.600002)
        (xy 122.199996 79.6)
        (xy 118.700003 79.6)
        (xy 118.700003 80.75001)
        (xy 118.900003 80.75001)
        (xy 118.900003 79.799999)
        (xy 119.900001 79.799999)
        (xy 119.900001 80.75001)
        (xy 120.1 80.75001)
        (xy 120.1 79.799999)
        (xy 121.099998 79.799999)
        (xy 121.099998 80.75001)
        (xy 121.299998 80.75001)
        (xy 121.299998 79.799999)
        (xy 122.199996 79.799999)
        (xy 122.199996 80.799997)
        (xy 118.700003 80.799997)
        (xy 118.700003 81.850008)
        (xy 118.900003 81.850008)
        (xy 118.900003 80.999997)
        (xy 119.900001 80.999997)
        (xy 119.900001 81.850008)
        (xy 120.1 81.850008)
        (xy 120.1 80.999997)
        (xy 121.099998 80.999997)
        (xy 121.099998 81.799995)
        (xy 121.099998 81.850008)
        (xy 121.299998 81.850008)
        (xy 121.299998 81.799995)
        (xy 121.299998 80.999997)
        (xy 122.199996 80.999997)
        (xy 122.199996 81.899995)
        (xy 120.4 81.899995)
        (xy 117.800005 81.899995)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.5449 98.655099)
        (xy 105.563499 98.7)
        (xy 105.5449 98.744901)
        (xy 105.499999 98.7635)
        (xy 102.999999 98.7635)
        (xy 102.955098 98.744901)
        (xy 102.936499 98.7)
        (xy 102.955098 98.655099)
        (xy 102.999999 98.6365)
        (xy 105.499999 98.6365)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.5449 99.655099)
        (xy 133.563499 99.7)
        (xy 133.5449 99.744901)
        (xy 133.499999 99.7635)
        (xy 106.499999 99.7635)
        (xy 106.455098 99.744901)
        (xy 106.436499 99.7)
        (xy 106.455098 99.655099)
        (xy 106.499999 99.6365)
        (xy 133.499999 99.6365)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.676393 87.614885)
        (xy 100.764886 87.526392)
        (xy 100.876393 87.469576)
        (xy 101 87.449999)
        (xy 101.123607 87.469576)
        (xy 101.235114 87.526392)
        (xy 101.323607 87.614885)
        (xy 101.380423 87.726392)
        (xy 101.4 87.849999)
        (xy 101.380423 87.973606)
        (xy 101.323607 88.085113)
        (xy 101.235114 88.173606)
        (xy 101.123607 88.230422)
        (xy 101 88.249999)
        (xy 100.876393 88.230422)
        (xy 100.764886 88.173606)
        (xy 100.676393 88.085113)
        (xy 100.619577 87.973606)
        (xy 100.6 87.849999)
        (xy 100.619577 87.726392)
      )
    )
    (polygon
      (pts
        (xy 100.766641 88.04581)
        (xy 100.847686 88.113815)
        (xy 100.947102 88.149999)
        (xy 101.052898 88.149999)
        (xy 101.152314 88.113815)
        (xy 101.233359 88.04581)
        (xy 101.286257 87.954188)
        (xy 101.304628 87.849999)
        (xy 101.286257 87.74581)
        (xy 101.233359 87.654188)
        (xy 101.152314 87.586183)
        (xy 101.052898 87.549999)
        (xy 100.947102 87.549999)
        (xy 100.847686 87.586183)
        (xy 100.766641 87.654188)
        (xy 100.713743 87.74581)
        (xy 100.695372 87.849999)
        (xy 100.713743 87.954188)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.388197 74.861644)
        (xy 104.474145 74.775696)
        (xy 104.582447 74.720514)
        (xy 104.7025 74.701499)
        (xy 104.822553 74.720514)
        (xy 104.930855 74.775696)
        (xy 105.016803 74.861644)
        (xy 105.071985 74.969946)
        (xy 105.091 75.089999)
        (xy 105.071985 75.210052)
        (xy 105.016803 75.318354)
        (xy 104.930855 75.404302)
        (xy 104.822553 75.459484)
        (xy 104.7025 75.478499)
        (xy 104.582447 75.459484)
        (xy 104.474145 75.404302)
        (xy 104.388197 75.318354)
        (xy 104.333015 75.210052)
        (xy 104.314 75.089999)
        (xy 104.333015 74.969946)
      )
    )
    (polygon
      (pts
        (xy 104.513969 75.27853)
        (xy 104.600468 75.336327)
        (xy 104.7025 75.356622)
        (xy 104.804532 75.336327)
        (xy 104.891031 75.27853)
        (xy 104.948828 75.192031)
        (xy 104.969123 75.089999)
        (xy 104.948828 74.987967)
        (xy 104.891031 74.901468)
        (xy 104.804532 74.843671)
        (xy 104.7025 74.823376)
        (xy 104.600468 74.843671)
        (xy 104.513969 74.901468)
        (xy 104.456172 74.987967)
        (xy 104.435877 75.089999)
        (xy 104.456172 75.192031)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.388197 89.861644)
        (xy 104.474145 89.775696)
        (xy 104.582447 89.720514)
        (xy 104.7025 89.701499)
        (xy 104.822553 89.720514)
        (xy 104.930855 89.775696)
        (xy 105.016803 89.861644)
        (xy 105.071985 89.969946)
        (xy 105.091 90.089999)
        (xy 105.071985 90.210052)
        (xy 105.016803 90.318354)
        (xy 104.930855 90.404302)
        (xy 104.822553 90.459484)
        (xy 104.7025 90.478499)
        (xy 104.582447 90.459484)
        (xy 104.474145 90.404302)
        (xy 104.388197 90.318354)
        (xy 104.333015 90.210052)
        (xy 104.314 90.089999)
        (xy 104.333015 89.969946)
      )
    )
    (polygon
      (pts
        (xy 104.513969 90.27853)
        (xy 104.600468 90.336327)
        (xy 104.7025 90.356622)
        (xy 104.804532 90.336327)
        (xy 104.891031 90.27853)
        (xy 104.948828 90.192031)
        (xy 104.969123 90.089999)
        (xy 104.948828 89.987967)
        (xy 104.891031 89.901468)
        (xy 104.804532 89.843671)
        (xy 104.7025 89.823376)
        (xy 104.600468 89.843671)
        (xy 104.513969 89.901468)
        (xy 104.456172 89.987967)
        (xy 104.435877 90.089999)
        (xy 104.456172 90.192031)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.499999 98.6365)
        (xy 134.544901 98.655098)
        (xy 134.563499 98.7)
        (xy 134.544901 98.744901)
        (xy 133.5449 99.744901)
        (xy 133.499999 99.7635)
        (xy 133.455098 99.744901)
        (xy 133.436499 99.7)
        (xy 133.455098 99.655099)
        (xy 134.455098 98.655098)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.955099 63.6551)
        (xy 100 63.636501)
        (xy 100.044901 63.6551)
        (xy 100.0635 63.700001)
        (xy 100.0635 71.200001)
        (xy 100.044901 71.244902)
        (xy 100 71.263501)
        (xy 99.955099 71.244902)
        (xy 99.9365 71.200001)
        (xy 99.9365 63.700001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.676393 89.314886)
        (xy 100.764886 89.226393)
        (xy 100.876393 89.169577)
        (xy 101 89.15)
        (xy 101.123607 89.169577)
        (xy 101.235114 89.226393)
        (xy 101.323607 89.314886)
        (xy 101.380423 89.426393)
        (xy 101.4 89.55)
        (xy 101.380423 89.673607)
        (xy 101.323607 89.785114)
        (xy 101.235114 89.873607)
        (xy 101.123607 89.930423)
        (xy 101 89.95)
        (xy 100.876393 89.930423)
        (xy 100.764886 89.873607)
        (xy 100.676393 89.785114)
        (xy 100.619577 89.673607)
        (xy 100.6 89.55)
        (xy 100.619577 89.426393)
      )
    )
    (polygon
      (pts
        (xy 100.766641 89.745811)
        (xy 100.847686 89.813816)
        (xy 100.947102 89.85)
        (xy 101.052898 89.85)
        (xy 101.152314 89.813816)
        (xy 101.233359 89.745811)
        (xy 101.286257 89.654189)
        (xy 101.304628 89.55)
        (xy 101.286257 89.445811)
        (xy 101.233359 89.354189)
        (xy 101.152314 89.286184)
        (xy 101.052898 89.25)
        (xy 100.947102 89.25)
        (xy 100.847686 89.286184)
        (xy 100.766641 89.354189)
        (xy 100.713743 89.445811)
        (xy 100.695372 89.55)
        (xy 100.713743 89.654189)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.676393 71.314887)
        (xy 100.764886 71.226394)
        (xy 100.876393 71.169578)
        (xy 101 71.150001)
        (xy 101.123607 71.169578)
        (xy 101.235114 71.226394)
        (xy 101.323607 71.314887)
        (xy 101.380423 71.426394)
        (xy 101.4 71.550001)
        (xy 101.380423 71.673608)
        (xy 101.323607 71.785115)
        (xy 101.235114 71.873608)
        (xy 101.123607 71.930424)
        (xy 101 71.950001)
        (xy 100.876393 71.930424)
        (xy 100.764886 71.873608)
        (xy 100.676393 71.785115)
        (xy 100.619577 71.673608)
        (xy 100.6 71.550001)
        (xy 100.619577 71.426394)
      )
    )
    (polygon
      (pts
        (xy 100.766641 71.745812)
        (xy 100.847686 71.813817)
        (xy 100.947102 71.850001)
        (xy 101.052898 71.850001)
        (xy 101.152314 71.813817)
        (xy 101.233359 71.745812)
        (xy 101.286257 71.65419)
        (xy 101.304628 71.550001)
        (xy 101.286257 71.445812)
        (xy 101.233359 71.35419)
        (xy 101.152314 71.286185)
        (xy 101.052898 71.250001)
        (xy 100.947102 71.250001)
        (xy 100.847686 71.286185)
        (xy 100.766641 71.35419)
        (xy 100.713743 71.445812)
        (xy 100.695372 71.550001)
        (xy 100.713743 71.65419)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.0449 95.6551)
        (xy 100.063499 95.700001)
        (xy 100.059424 95.709838)
        (xy 100.077365 96.029303)
        (xy 100.132612 96.354463)
        (xy 100.223918 96.671394)
        (xy 100.350135 96.976108)
        (xy 100.509676 97.264775)
        (xy 100.700534 97.533763)
        (xy 100.920308 97.779692)
        (xy 101.166237 97.999466)
        (xy 101.435225 98.190324)
        (xy 101.723892 98.349865)
        (xy 102.028606 98.476082)
        (xy 102.345537 98.567388)
        (xy 102.670697 98.622635)
        (xy 102.990162 98.640576)
        (xy 102.999999 98.636501)
        (xy 103.0449 98.6551)
        (xy 103.063499 98.700001)
        (xy 103.0449 98.744902)
        (xy 102.999999 98.763501)
        (xy 102.679776 98.746719)
        (xy 102.363062 98.696556)
        (xy 102.053326 98.613562)
        (xy 101.753961 98.498647)
        (xy 101.468249 98.35307)
        (xy 101.199319 98.178424)
        (xy 100.950118 97.976625)
        (xy 100.723375 97.749882)
        (xy 100.521576 97.500681)
        (xy 100.34693 97.231751)
        (xy 100.201353 96.946039)
        (xy 100.086438 96.646674)
        (xy 100.003444 96.336938)
        (xy 99.953281 96.020224)
        (xy 99.936499 95.700001)
        (xy 99.955098 95.6551)
        (xy 99.999999 95.636501)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.388197 69.081645)
        (xy 104.474145 68.995697)
        (xy 104.582447 68.940515)
        (xy 104.7025 68.9215)
        (xy 104.822553 68.940515)
        (xy 104.930855 68.995697)
        (xy 105.016803 69.081645)
        (xy 105.071985 69.189947)
        (xy 105.091 69.31)
        (xy 105.071985 69.430053)
        (xy 105.016803 69.538355)
        (xy 104.930855 69.624303)
        (xy 104.822553 69.679485)
        (xy 104.7025 69.6985)
        (xy 104.582447 69.679485)
        (xy 104.474145 69.624303)
        (xy 104.388197 69.538355)
        (xy 104.333015 69.430053)
        (xy 104.314 69.31)
        (xy 104.333015 69.189947)
      )
    )
    (polygon
      (pts
        (xy 104.513969 69.498531)
        (xy 104.600468 69.556328)
        (xy 104.7025 69.576623)
        (xy 104.804532 69.556328)
        (xy 104.891031 69.498531)
        (xy 104.948828 69.412032)
        (xy 104.969123 69.31)
        (xy 104.948828 69.207968)
        (xy 104.891031 69.121469)
        (xy 104.804532 69.063672)
        (xy 104.7025 69.043377)
        (xy 104.600468 69.063672)
        (xy 104.513969 69.121469)
        (xy 104.456172 69.207968)
        (xy 104.435877 69.31)
        (xy 104.456172 69.412032)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.373362 72.402618)
        (xy 110.373362 70.201708)
        (xy 109.97458 70.20171)
        (xy 109.97458 69.20222)
        (xy 109.42213 69.20222)
        (xy 108.87349 69.20222)
        (xy 108.87349 70.20171)
        (xy 108.473442 70.20171)
        (xy 108.473442 72.40262)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.320222 60.653283)
        (xy 137.636936 60.703446)
        (xy 137.946672 60.78644)
        (xy 138.246037 60.901355)
        (xy 138.531749 61.046932)
        (xy 138.800679 61.221578)
        (xy 139.04988 61.423377)
        (xy 139.276623 61.65012)
        (xy 139.478422 61.899321)
        (xy 139.653068 62.168251)
        (xy 139.798645 62.453963)
        (xy 139.91356 62.753328)
        (xy 139.996554 63.063064)
        (xy 140.046717 63.379778)
        (xy 140.063499 63.700001)
        (xy 140.0449 63.744902)
        (xy 139.999999 63.763501)
        (xy 139.955098 63.744902)
        (xy 139.936499 63.700001)
        (xy 139.940574 63.690164)
        (xy 139.922633 63.370699)
        (xy 139.867386 63.045539)
        (xy 139.77608 62.728608)
        (xy 139.649863 62.423894)
        (xy 139.490322 62.135227)
        (xy 139.299464 61.866239)
        (xy 139.07969 61.62031)
        (xy 138.833761 61.400536)
        (xy 138.564773 61.209678)
        (xy 138.276106 61.050137)
        (xy 137.971392 60.92392)
        (xy 137.654461 60.832614)
        (xy 137.329301 60.777367)
        (xy 137.009836 60.759426)
        (xy 136.999999 60.763501)
        (xy 136.955098 60.744902)
        (xy 136.936499 60.700001)
        (xy 136.955098 60.6551)
        (xy 136.999999 60.636501)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.955099 77.5551)
        (xy 100 77.536501)
        (xy 100.044901 77.5551)
        (xy 100.0635 77.600001)
        (xy 100.0635 95.700001)
        (xy 100.044901 95.744902)
        (xy 100 95.763501)
        (xy 99.955099 95.744902)
        (xy 99.9365 95.700001)
        (xy 99.9365 77.600001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.044899 95.744902)
        (xy 139.999998 95.763501)
        (xy 139.955097 95.744902)
        (xy 139.936498 95.700001)
        (xy 139.936496 63.700001)
        (xy 139.955095 63.6551)
        (xy 139.999996 63.636501)
        (xy 140.044897 63.6551)
        (xy 140.063496 63.700001)
        (xy 140.063498 95.700001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.0449 60.6551)
        (xy 103.063499 60.700001)
        (xy 103.0449 60.744902)
        (xy 102.999999 60.763501)
        (xy 102.990162 60.759426)
        (xy 102.670697 60.777367)
        (xy 102.345537 60.832614)
        (xy 102.028606 60.92392)
        (xy 101.723892 61.050137)
        (xy 101.435225 61.209678)
        (xy 101.166237 61.400536)
        (xy 100.920308 61.62031)
        (xy 100.700534 61.866239)
        (xy 100.509676 62.135227)
        (xy 100.350135 62.423894)
        (xy 100.223918 62.728608)
        (xy 100.132612 63.045539)
        (xy 100.077365 63.370699)
        (xy 100.059424 63.690164)
        (xy 100.063499 63.700001)
        (xy 100.0449 63.744902)
        (xy 99.999999 63.763501)
        (xy 99.955098 63.744902)
        (xy 99.936499 63.700001)
        (xy 99.953281 63.379778)
        (xy 100.003444 63.063064)
        (xy 100.086438 62.753328)
        (xy 100.201353 62.453963)
        (xy 100.34693 62.168251)
        (xy 100.521576 61.899321)
        (xy 100.723375 61.65012)
        (xy 100.950118 61.423377)
        (xy 101.199319 61.221578)
        (xy 101.468249 61.046932)
        (xy 101.753961 60.901355)
        (xy 102.053326 60.78644)
        (xy 102.363062 60.703446)
        (xy 102.679776 60.653283)
        (xy 102.999999 60.636501)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.955099 71.1551)
        (xy 100 71.136501)
        (xy 100.044901 71.1551)
        (xy 100.0635 71.200001)
        (xy 100.0635 77.600001)
        (xy 100.044901 77.644902)
        (xy 100 77.663501)
        (xy 99.955099 77.644902)
        (xy 99.9365 77.600001)
        (xy 99.9365 71.200001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.563499 99.7)
        (xy 106.544901 99.744902)
        (xy 106.499999 99.7635)
        (xy 106.455098 99.744902)
        (xy 105.455098 98.744901)
        (xy 105.436499 98.7)
        (xy 105.455098 98.655099)
        (xy 105.499999 98.6365)
        (xy 105.5449 98.655099)
        (xy 106.544901 99.655099)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.388197 84.081646)
        (xy 104.474145 83.995698)
        (xy 104.582447 83.940516)
        (xy 104.7025 83.921501)
        (xy 104.822553 83.940516)
        (xy 104.930855 83.995698)
        (xy 105.016803 84.081646)
        (xy 105.071985 84.189948)
        (xy 105.091 84.310001)
        (xy 105.071985 84.430054)
        (xy 105.016803 84.538356)
        (xy 104.930855 84.624304)
        (xy 104.822553 84.679486)
        (xy 104.7025 84.698501)
        (xy 104.582447 84.679486)
        (xy 104.474145 84.624304)
        (xy 104.388197 84.538356)
        (xy 104.333015 84.430054)
        (xy 104.314 84.310001)
        (xy 104.333015 84.189948)
      )
    )
    (polygon
      (pts
        (xy 104.513969 84.498532)
        (xy 104.600468 84.556329)
        (xy 104.7025 84.576624)
        (xy 104.804532 84.556329)
        (xy 104.891031 84.498532)
        (xy 104.948828 84.412033)
        (xy 104.969123 84.310001)
        (xy 104.948828 84.207969)
        (xy 104.891031 84.12147)
        (xy 104.804532 84.063673)
        (xy 104.7025 84.043378)
        (xy 104.600468 84.063673)
        (xy 104.513969 84.12147)
        (xy 104.456172 84.207969)
        (xy 104.435877 84.310001)
        (xy 104.456172 84.412033)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.676393 69.614885)
        (xy 100.764886 69.526392)
        (xy 100.876393 69.469576)
        (xy 101 69.449999)
        (xy 101.123607 69.469576)
        (xy 101.235114 69.526392)
        (xy 101.323607 69.614885)
        (xy 101.380423 69.726392)
        (xy 101.4 69.849999)
        (xy 101.380423 69.973606)
        (xy 101.323607 70.085113)
        (xy 101.235114 70.173606)
        (xy 101.123607 70.230422)
        (xy 101 70.249999)
        (xy 100.876393 70.230422)
        (xy 100.764886 70.173606)
        (xy 100.676393 70.085113)
        (xy 100.619577 69.973606)
        (xy 100.6 69.849999)
        (xy 100.619577 69.726392)
      )
    )
    (polygon
      (pts
        (xy 100.766641 70.04581)
        (xy 100.847686 70.113815)
        (xy 100.947102 70.149999)
        (xy 101.052898 70.149999)
        (xy 101.152314 70.113815)
        (xy 101.233359 70.04581)
        (xy 101.286257 69.954188)
        (xy 101.304628 69.849999)
        (xy 101.286257 69.74581)
        (xy 101.233359 69.654188)
        (xy 101.152314 69.586183)
        (xy 101.052898 69.549999)
        (xy 100.947102 69.549999)
        (xy 100.847686 69.586183)
        (xy 100.766641 69.654188)
        (xy 100.713743 69.74581)
        (xy 100.695372 69.849999)
        (xy 100.713743 69.954188)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.5449 60.655101)
        (xy 105.563499 60.700002)
        (xy 105.5449 60.744903)
        (xy 105.499999 60.763502)
        (xy 102.999999 60.763502)
        (xy 102.955098 60.744903)
        (xy 102.936499 60.700002)
        (xy 102.955098 60.655101)
        (xy 102.999999 60.636502)
        (xy 105.499999 60.636502)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.563499 60.700002)
        (xy 134.544901 60.744904)
        (xy 134.499999 60.763502)
        (xy 134.455098 60.744904)
        (xy 133.455098 59.744903)
        (xy 133.436499 59.700002)
        (xy 133.455098 59.655101)
        (xy 133.499999 59.636502)
        (xy 133.5449 59.655101)
        (xy 134.544901 60.655101)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.499999 59.636502)
        (xy 106.544901 59.6551)
        (xy 106.563499 59.700002)
        (xy 106.544901 59.744903)
        (xy 105.5449 60.744903)
        (xy 105.499999 60.763502)
        (xy 105.455098 60.744903)
        (xy 105.436499 60.700002)
        (xy 105.455098 60.655101)
        (xy 106.455098 59.6551)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.5449 59.655101)
        (xy 133.563499 59.700002)
        (xy 133.5449 59.744903)
        (xy 133.499999 59.763502)
        (xy 106.499999 59.763502)
        (xy 106.455098 59.744903)
        (xy 106.436499 59.700002)
        (xy 106.455098 59.655101)
        (xy 106.499999 59.636502)
        (xy 133.499999 59.636502)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.0449 98.655099)
        (xy 137.063499 98.7)
        (xy 137.0449 98.744901)
        (xy 136.999999 98.7635)
        (xy 134.499999 98.7635)
        (xy 134.455098 98.744901)
        (xy 134.436499 98.7)
        (xy 134.455098 98.655099)
        (xy 134.499999 98.6365)
        (xy 136.999999 98.6365)
      )
    )
  )
  (zone (net 128) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 133.075567 59.983598)
        (xy 133.139049 60.060951)
        (xy 134.13905 61.060951)
        (xy 134.216403 61.124434)
        (xy 134.304655 61.171604)
        (xy 134.400413 61.200654)
        (xy 134.499999 61.210461)
        (xy 136.999971 61.210461)
        (xy 136.999997 61.210463)
        (xy 137.016116 61.208876)
        (xy 137.217174 61.217654)
        (xy 137.432699 61.246028)
        (xy 137.644931 61.293079)
        (xy 137.852253 61.358449)
        (xy 138.053088 61.441636)
        (xy 138.245913 61.542015)
        (xy 138.429252 61.658814)
        (xy 138.601713 61.791151)
        (xy 138.761987 61.938011)
        (xy 138.908847 62.098285)
        (xy 139.041184 62.270746)
        (xy 139.157983 62.454088)
        (xy 139.258362 62.64691)
        (xy 139.341549 62.847745)
        (xy 139.406919 63.055067)
        (xy 139.45397 63.267299)
        (xy 139.482344 63.482824)
        (xy 139.491122 63.683885)
        (xy 139.489535 63.700001)
        (xy 139.489537 63.700027)
        (xy 139.48954 95.700001)
        (xy 139.491127 95.716117)
        (xy 139.482349 95.917178)
        (xy 139.453975 96.132702)
        (xy 139.406924 96.344935)
        (xy 139.341554 96.552257)
        (xy 139.258367 96.753095)
        (xy 139.157988 96.945916)
        (xy 139.041189 97.129256)
        (xy 138.908853 97.30172)
        (xy 138.76199 97.461991)
        (xy 138.601718 97.608854)
        (xy 138.429255 97.74119)
        (xy 138.245915 97.85799)
        (xy 138.053093 97.958368)
        (xy 137.852256 98.041556)
        (xy 137.644933 98.106925)
        (xy 137.432701 98.153976)
        (xy 137.217177 98.18235)
        (xy 137.016116 98.191129)
        (xy 136.999999 98.189541)
        (xy 134.499999 98.189541)
        (xy 134.400413 98.199348)
        (xy 134.304655 98.228398)
        (xy 134.216403 98.275568)
        (xy 134.13905 98.339051)
        (xy 133.139049 99.339051)
        (xy 133.075567 99.416404)
        (xy 133.036477 99.489541)
        (xy 106.963521 99.489541)
        (xy 106.924431 99.416404)
        (xy 106.860949 99.339051)
        (xy 105.860948 98.339051)
        (xy 105.783595 98.275568)
        (xy 105.695343 98.228398)
        (xy 105.599585 98.199348)
        (xy 105.499999 98.189541)
        (xy 102.999999 98.189541)
        (xy 102.983882 98.191129)
        (xy 102.782821 98.18235)
        (xy 102.567297 98.153976)
        (xy 102.355065 98.106925)
        (xy 102.147742 98.041556)
        (xy 101.946905 97.958368)
        (xy 101.754083 97.85799)
        (xy 101.570743 97.74119)
        (xy 101.39828 97.608854)
        (xy 101.238008 97.461991)
        (xy 101.091146 97.30172)
        (xy 100.958809 97.129256)
        (xy 100.84201 96.945916)
        (xy 100.741631 96.753095)
        (xy 100.658444 96.552257)
        (xy 100.593074 96.344935)
        (xy 100.546023 96.132702)
        (xy 100.517649 95.917178)
        (xy 100.508871 95.716117)
        (xy 100.510458 95.700001)
        (xy 100.510458 63.700001)
        (xy 100.508871 63.683885)
        (xy 100.517649 63.482824)
        (xy 100.546023 63.267299)
        (xy 100.593074 63.055067)
        (xy 100.658444 62.847745)
        (xy 100.741631 62.646907)
        (xy 100.84201 62.454085)
        (xy 100.958809 62.270746)
        (xy 101.091146 62.098282)
        (xy 101.238008 61.938011)
        (xy 101.39828 61.791148)
        (xy 101.570743 61.658811)
        (xy 101.754083 61.542012)
        (xy 101.946905 61.441634)
        (xy 102.147742 61.358446)
        (xy 102.355065 61.293077)
        (xy 102.567297 61.246026)
        (xy 102.782821 61.217652)
        (xy 102.983882 61.208873)
        (xy 102.999999 61.210461)
        (xy 105.499999 61.210461)
        (xy 105.599585 61.200654)
        (xy 105.695343 61.171604)
        (xy 105.783595 61.124434)
        (xy 105.860948 61.060951)
        (xy 106.860949 60.060951)
        (xy 106.924431 59.983598)
        (xy 106.963524 59.910458)
        (xy 133.036474 59.910458)
      )
    )
  )
  (zone (net 128) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 106.7256 59.9744)
        (xy 133.274397 59.9744)
        (xy 139.5732 66.273202)
        (xy 139.5732 93.1468)
        (xy 139.5532 93.1468)
        (xy 133.4826 99.2174)
        (xy 106.517397 99.2174)
        (xy 100.508 93.208002)
        (xy 100.508 66.192)
      )
    )
  )
)
