(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
  )
  (sheet (at 80.01 92.71) (size 30.48 21.59) (fields_autoplaced)
    (fill (color 0 0 0 0.0000))
    (property "Sheet name" "D1s" (id 0) (at 80.01 91.9984 0))
    (property "Sheet file" "D1s.kicad_sch" (id 1) (at 80.01 114.8846 0))
  )
  (sheet (at 129.54 92.71) (size 31.75 20.32) (fields_autoplaced)
    (fill (color 0 0 0 0.0000))
    (property "Sheet name" "Periph" (id 0) (at 129.54 91.9984 0))
    (property "Sheet file" "Periph.kicad_sch" (id 1) (at 129.54 113.6146 0))
  )
  (sheet (at 171.45 92.71) (size 36.83 19.05)
    (fill (color 0 0 0 0.0000))
    (property "Sheet name" "WIFI" (id 0) (at 171.45 91.9984 0))
    (property "Sheet file" "WIFI-BT.kicad_sch" (id 1) (at 172.72 113.03 0))
  )
  (sheet_instances
    (path (page "1"))
    (path (page "1"))
    (path (page "3"))
    (path (page "4"))
  )
  (symbol_instances
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-CORE") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-CORE") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-CORE") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-DRAM") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AVCC1.8") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-CORE") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCCIN") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-CORE") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC_WIFI") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AVDD2V8") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCCIN") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AVDD2V8") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCCIN") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-RMII-CSI") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCCIN") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-RMII-CSI") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCCIN") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AAGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AVDD2V8") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "AAGND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCCIN") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-RMII-CSI") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC-CORE") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "1uF 50V") (footprint "C0603")
    )
    (path
      (reference "C2") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C3") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C4") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C5") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C6") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C7") (unit 1) (value "100pF") (footprint "C0402")
    )
    (path
      (reference "C8") (unit 1) (value "22pF") (footprint "C0402")
    )
    (path
      (reference "C9") (unit 1) (value "22pF") (footprint "C0402")
    )
    (path
      (reference "C10") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C11") (unit 1) (value "2.2uF") (footprint "C0402")
    )
    (path
      (reference "C12") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C13") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C14") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C16") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C18") (unit 1) (value "NC") (footprint "C0402")
    )
    (path
      (reference "C19") (unit 1) (value "1uF") (footprint "C0402")
    )
    (path
      (reference "C20") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C21") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C22") (unit 1) (value "2.2uF") (footprint "C0402")
    )
    (path
      (reference "C23") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C24") (unit 1) (value "1uF") (footprint "C0402")
    )
    (path
      (reference "C25") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C26") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C27") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C28") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C29") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C30") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C31") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C32") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C33") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C34") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C35") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C36") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C37") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C38") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C39") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C40") (unit 1) (value "0.47uF") (footprint "C0402")
    )
    (path
      (reference "C41") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C42") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C43") (unit 1) (value "22pF") (footprint "C0402")
    )
    (path
      (reference "C44") (unit 1) (value "2.2uF") (footprint "C0402")
    )
    (path
      (reference "C45") (unit 1) (value "22pF") (footprint "C0402")
    )
    (path
      (reference "C46") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C47") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C48") (unit 1) (value "NC") (footprint "C0402")
    )
    (path
      (reference "C49") (unit 1) (value "1nF") (footprint "C0402")
    )
    (path
      (reference "C50") (unit 1) (value "2.2uF") (footprint "C0402")
    )
    (path
      (reference "C51") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C52") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C53") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C54") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C55") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C58") (unit 1) (value "NC") (footprint "C0402")
    )
    (path
      (reference "C59") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C60") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C61") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C62") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C63") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C64") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C65") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C66") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C67") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C68") (unit 1) (value "2.2uF") (footprint "C0402")
    )
    (path
      (reference "C69") (unit 1) (value "1uF") (footprint "C0402")
    )
    (path
      (reference "C70") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C71") (unit 1) (value "1uF") (footprint "C0402")
    )
    (path
      (reference "C72") (unit 1) (value "1nF") (footprint "C0402")
    )
    (path
      (reference "C73") (unit 1) (value "1nF") (footprint "C0402")
    )
    (path
      (reference "C74") (unit 1) (value "1nF") (footprint "C0402")
    )
    (path
      (reference "C75") (unit 1) (value "1nF") (footprint "C0402")
    )
    (path
      (reference "C76") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C77") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C78") (unit 1) (value "0.47uF") (footprint "C0402")
    )
    (path
      (reference "C79") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C80") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C81") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C82") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C83") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C84") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C85") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C86") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "D1") (unit 1) (value "MSK4010") (footprint "SOD523")
    )
    (path
      (reference "D2") (unit 1) (value "MSK4010") (footprint "SOD523")
    )
    (path
      (reference "DS1") (unit 1) (value "GREEN") (footprint "LED0402")
    )
    (path
      (reference "DS2") (unit 1) (value "BLUE") (footprint "LED0402")
    )
    (path
      (reference "J1") (unit 1) (value "TF5033981892") (footprint "TFCARD-1040310811")
    )
    (path
      (reference "J2") (unit 1) (value "USB-TypeC-16P") (footprint "usb-typec-16p")
    )
    (path
      (reference "J3") (unit 1) (value "USB-TypeC-16P") (footprint "usb-typec-16p")
    )
    (path
      (reference "J4") (unit 1) (value "ipex") (footprint "I-PEX SOCKET")
    )
    (path
      (reference "L1") (unit 1) (value "2.2uH") (footprint "VLS2016")
    )
    (path
      (reference "L2") (unit 1) (value "2.2uH") (footprint "VLS2016")
    )
    (path
      (reference "L3") (unit 1) (value "2.2uH") (footprint "VLS2016")
    )
    (path
      (reference "L4") (unit 1) (value "10uH") (footprint "VLS252010")
    )
    (path
      (reference "M1") (unit 1) (value "MIC") (footprint "MIC")
    )
    (path
      (reference "P1") (unit 1) (value "FFC40-RGBLCD") (footprint "FFC/SM0.5-1H40")
    )
    (path
      (reference "P2") (unit 1) (value "Header 11X2") (footprint "HDR2X11T")
    )
    (path
      (reference "P3") (unit 1) (value "Header 11X2") (footprint "HDR2X11T")
    )
    (path
      (reference "P4") (unit 1) (value "FPC6") (footprint "FPC6")
    )
    (path
      (reference "P5") (unit 1) (value "Header15-MIPI") (footprint "MIPI_CSI_1.0_30PIN")
    )
    (path
      (reference "P6") (unit 1) (value "Header 4") (footprint "HDR1.27-4")
    )
    (path
      (reference "P8") (unit 1) (value "Header 3") (footprint "HDR1.27-3")
    )
    (path
      (reference "R1") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R2") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R3") (unit 1) (value "33R") (footprint "R0402")
    )
    (path
      (reference "R4") (unit 1) (value "2R7") (footprint "R0402")
    )
    (path
      (reference "R5") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R6") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R7") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R8") (unit 1) (value "680K 1%") (footprint "R0402")
    )
    (path
      (reference "R9") (unit 1) (value "150K 1%") (footprint "R0402")
    )
    (path
      (reference "R10") (unit 1) (value "300K 1%") (footprint "R0402")
    )
    (path
      (reference "R11") (unit 1) (value "150K 1%") (footprint "R0402")
    )
    (path
      (reference "R12") (unit 1) (value "75K 1%") (footprint "R0402")
    )
    (path
      (reference "R13") (unit 1) (value "150K 1%") (footprint "R0402")
    )
    (path
      (reference "R14") (unit 1) (value "NC/100K") (footprint "R0402")
    )
    (path
      (reference "R15") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R16") (unit 1) (value "75R") (footprint "R0402")
    )
    (path
      (reference "R17") (unit 1) (value "75R") (footprint "R0402")
    )
    (path
      (reference "R18") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R23") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R24") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R25") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R26") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R27") (unit 1) (value "1K") (footprint "R0402")
    )
    (path
      (reference "R28") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R29") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R30") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R32") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R33") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R34") (unit 1) (value "1K") (footprint "R0402")
    )
    (path
      (reference "R35") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R36") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R37") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R38") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R39") (unit 1) (value "33R") (footprint "R0402")
    )
    (path
      (reference "R40") (unit 1) (value "680K 1%") (footprint "R0402")
    )
    (path
      (reference "R41") (unit 1) (value "NC/0R") (footprint "R0402")
    )
    (path
      (reference "R42") (unit 1) (value "240R 1%") (footprint "R0402")
    )
    (path
      (reference "R43") (unit 1) (value "33R") (footprint "R0402")
    )
    (path
      (reference "R45") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R46") (unit 1) (value "NC/100K") (footprint "R0402")
    )
    (path
      (reference "R47") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R48") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R49") (unit 1) (value "33R") (footprint "R0402")
    )
    (path
      (reference "R50") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R52") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R53") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R54") (unit 1) (value "NC/1K") (footprint "R0402")
    )
    (path
      (reference "R55") (unit 1) (value "75R") (footprint "R0402")
    )
    (path
      (reference "R56") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R57") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R58") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R59") (unit 1) (value "33R") (footprint "R0402")
    )
    (path
      (reference "R60") (unit 1) (value "75R") (footprint "R0402")
    )
    (path
      (reference "R61") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R64") (unit 1) (value "33R") (footprint "R0402")
    )
    (path
      (reference "R65") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R66") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R67") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R68") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R69") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R70") (unit 1) (value "NC/100K") (footprint "R0402")
    )
    (path
      (reference "R71") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R72") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R73") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R74") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R75") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R76") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R77") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "R78") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R79") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R80") (unit 1) (value "5.1K") (footprint "R0402")
    )
    (path
      (reference "R81") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R82") (unit 1) (value "10K") (footprint "R0402")
    )
    (path
      (reference "R84") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "S1") (unit 1) (value "SW-CE") (footprint "miniSW")
    )
    (path
      (reference "S2") (unit 1) (value "SW-CE") (footprint "miniSW")
    )
    (path
      (reference "TP1") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "TP2") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "TP3") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "TP4") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "TP5") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "TP6") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "TP7") (unit 1) (value "TEST POINT") (footprint "TEST-POINT")
    )
    (path
      (reference "U1") (unit 1) (value "D1s-eLQFP128") (footprint "QFP129P40B1600_1600H160")
    )
    (path
      (reference "U2") (unit 1) (value "XC6206-1.8V") (footprint "SOT23")
    )
    (path
      (reference "U3") (unit 1) (value "SPIFLASH_SOP8W") (footprint "WSON-SPIFLASH")
    )
    (path
      (reference "U4") (unit 1) (value "RY1303") (footprint "QFN40P300X300X80_HS-21N")
    )
    (path
      (reference "U5") (unit 1) (value "MT9284-28J") (footprint "SOT23-6")
    )
    (path
      (reference "U6") (unit 1) (value "WIFI") (footprint "AP6212")
    )
    (path
      (reference "U7") (unit 1) (value "OV-DVP") (footprint "FFC/SM0.5-2H24-OV5640")
    )
    (path
      (reference "U8") (unit 1) (value "XC6206-1.2") (footprint "SOT23")
    )
    (path
      (reference "U9") (unit 1) (value "XC6206-2.8") (footprint "SOT23")
    )
    (path
      (reference "X1") (unit 1) (value "XTAL2520-24M CL=18PF") (footprint "XTAL2520")
    )
    (path
      (reference "XT1") (unit 1) (value "32.768K CL=12.5pF") (footprint "Y3215")
    )
  )
)
